Product         GlyphWorks V25.0.0 Release Build 431
Platform        Windows64
abcdlib         V25.0 A01 Jan 14 2025 12:42:50
ailib           V25.0 A01 Jan 14 2025 12:43:34
Ans.DesignLifeAddin V25.1 A00 Tuesday, January 14, 2025 1:48:14 PM
anslib          V25.0 A01 Jan 14 2025 12:43:19
asamlib         V25.0 A01 Jan 14 2025 13:07:33
atlib           V25.0 A01 Jan 14 2025 12:51:03
CBLib           V25.0 A01 Jan 14 2025 12:43:46
cgdlib          V25.0 A01 Jan 14 2025 12:48:23
cgflib          V25.0 A01 Jan 14 2025 12:41:16
cgolib          V25.0 A01 Jan 14 2025 12:48:07
cgrlib          V25.0 A01 Jan 14 2025 12:47:43
cpputil         V25.0 A01 Jan 14 2025 12:34:31
dglib           V25.0 A01 Jan 14 2025 12:50:00
dmilib          V25.0 A01 Jan 14 2025 12:35:37
dtlib           V25.0 A01 Jan 14 2025 12:47:07
extlib          V25.0 A01 Jan 14 2025 12:32:12
fatlib          V25.0 A01 Jan 14 2025 12:39:41
FDLib           V25.0 A01 Jan 14 2025 12:44:23
fedlib          V25.0 A01 Jan 14 2025 12:53:52
feilib          V25.0 A01 Jan 14 2025 12:43:08
feimportlib (ANSYS) V25.0 A01 Jan 14 2025 12:46:38
ferlib          V25.0 A01 Jan 14 2025 12:37:58
fiolib          V25.0 A01 Jan 14 2025 12:42:00
FSLib           V25.0 A01 Jan 14 2025 12:37:05
FVLib           V25.0 A01 Jan 14 2025 12:56:58
GlyphEngine01   V25.0 A01 Jan 14 2025 12:59:10
GlyphEngine02   V25.0 A01 Jan 14 2025 12:59:49
GlyphEngine03   V25.0 A01 Jan 14 2025 13:00:38
GlyphEngine04   V25.0 A01 Jan 14 2025 13:01:39
GlyphEngine06   V25.0 A01 Jan 14 2025 13:02:36
GlyphEngine07   V25.0 A01 Jan 14 2025 13:03:02
GlyphEngine08   V25.0 A01 Jan 14 2025 13:03:23
GlyphEngine09   V25.0 A01 Jan 14 2025 13:03:48
GlyphEngine10   V25.0 A01 Jan 14 2025 13:04:14
GlyphEngine13   V25.0 A01 Jan 14 2025 13:04:39
GlyphEngine14   V25.0 A01 Jan 14 2025 13:05:28
GlyphEngine15   V25.0 A01 Jan 14 2025 13:05:56
GlyphEngine16   V25.0 A01 Jan 14 2025 13:06:24
grlib           V25.0 A01 Jan 14 2025 12:51:53
gutlib          V25.0 A01 Jan 14 2025 12:55:50
iceintlib       V25.0 A01 Jan 14 2025 12:50:33
IXDLib          V25.0 A01 Jan 14 2025 12:35:52
jprolib         V25.0 A01 Jan 14 2025 12:42:35
lican           V25.0 A01 Jan 14 2025 12:30:34
licnc           V25.0 A01 Jan 14 2025 12:30:19
licsh           V25.0 A01 Jan 14 2025 12:30:10
maplib          V25.0 A01 Jan 14 2025 12:35:25
matdblib        V25.0 A01 Jan 14 2025 12:38:15
materials       V25.0 A01 Jan 14 2025 12:49:26
mcxlib          V25.0 A01 Jan 14 2025 12:32:51
mthlib          V25.0 A01 Jan 14 2025 12:35:14
mtlib           V25.0 A01 Jan 14 2025 12:33:48
ncmpilib        V25.0 A01 Jan 14 2025 12:32:18
ncodedesktop    V25.0 A01 Jan 14 2025 13:27:32
ncxml           V25.0 A01 Jan 14 2025 12:30:42
nmxfiolib       V25.0 A01 Jan 14 2025 12:37:45
nulib           V25.0 A01 Jan 14 2025 12:34:46
NXLib           V25.0 A01 Jan 14 2025 12:33:01
PipeData00      V25.0 A01 Jan 14 2025 12:55:01
ProgramEngine00 V25.0 A01 Jan 14 2025 13:06:46
pylib           V25.0 A01 Jan 14 2025 12:33:57
QCLib           V25.0 A01 Jan 14 2025 12:55:21
qtutil          V25.0 A01 Jan 14 2025 12:48:50
QXLib           V25.0 A01 Jan 14 2025 12:45:08
S3Lib           V25.0 A01 Jan 14 2025 12:33:22
sielib          V25.0 A01 Jan 14 2025 12:37:35
siglib          V25.0 A01 Jan 14 2025 12:40:54
utlib (ANSYS)   V25.0 A01 Jan 14 2025 12:28:47
xllib           V25.0 A01 Jan 14 2025 12:31:01
Pre run audit data
   
Start time - 15-Aug-2025 15:15:56
Single run
Flow file - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-2\DL\dl.fdb
Glyph count - 17
   
   
Glyph 1 - "VibrationGenerator1"
Version - 5
   
Output connections - 1
Output connection 1:1 - Plug1.Vibration Profile to SweptSine_Analysis.Histogram.HistogramPipe1
Output connection 1:2 - Plug1.Vibration Profile to Swept Sine Display.HistSocket.s1b
   
Properties - 19 entries (pre-run state)
AdditionalNumberOfSweeps = 0
EndFrequency = 101
FrequencyStep = 1
InterpolationMethod = Log
Name = sine_sweep
NoiseFloor = -120
NumberOfBins = 1024
PSDUnits = Acceleration
SineAmplitudes = Undefined
SineFrequencies = Undefined
StartFrequency = 1
SweepRate = 1
SweepType = HZ/Sec (Linear)
TestDuration = 100
TestName = Undefined
TestType = Acceleration (g)
Type = SineSweep2
VibrationTable = PropertiesTab
XMLTables = <VibrationTables Version="1.0"><Tables><SineSweep/><SineDwell/><RandomPSD><RandomPSDItem Amplitude="1" Frequency="1"/><RandomPSDItem Amplitude="1" Frequency="1000"/></RandomPSD><SineOnRandom/><SineSweep2><SineSweep2Item Amplitude="0.1" Frequency="1"/><SineSweep2Item Amplitude="1" Frequency="10"/><SineSweep2Item Amplitude="1" Frequency="100"/></SineSweep2></Tables></VibrationTables>

   
   
Glyph 2 - "Bill_of_Materials_Input"
Version - 7
   
Input files - 1
Input file 1 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-2\DL\dlbom.csv;amc;c1
   
Output connections - 1
Output connection 1:1 - Plug1.P1a to SweptSine_Analysis.MaterialMapLoader.Use materials from Workbench
   
Properties - 7 entries (pre-run state)
CombineAllTests = False
DiscardProcessedTests = False
LoopAllTests = True
MatchingMethod = ChannelNumber
SVDecimalSeparator = 
SVSeparator = 
SaveTestList = False
   
   
Glyph 3 - "Simulation_Input"
Version - 8
   
Input files - 2
Input file 1 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\MECH\file.rst;afe;c1
Input file 2 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-1\MECH\file.rst;afe;c1
   
Output connections - 1
Output connection 1:1 - Plug1.FE Model Data to SweptSine_Analysis.FEMetaData.FRF Input
Output connection 1:2 - Plug1.FE Model Data to SweptSine_Analysis.FEMetaData.Offset Loadcase Input
   
Properties - 9 entries (pre-run state)
CombineTests = True
DiscardProcessedTests = False
ImportUserGroups = False
LoadCaseNumbering = EachFile
LoadCases = Undefined
LoopAllTests = True
SaveTestList = False
StoreDisplayedGroups = False
UserGroupsFilename = Undefined
   
   
Unable to locate glyph 3 name property in run 0 audit
Unable to locate glyph 3 version property in run 0 audit
Unable to locate glyph 3 input file count property in run 0 audit
Unable to locate glyph 3 input connection count property in run 0 audit
Unable to locate glyph 3 output connection count property in run 0 audit
Unable to locate glyph 3 pre-run property set in run 0 audit
   
   
Unable to locate glyph 4 name property in run 0 audit
Unable to locate glyph 4 version property in run 0 audit
Unable to locate glyph 4 input file count property in run 0 audit
Unable to locate glyph 4 input connection count property in run 0 audit
Unable to locate glyph 4 output connection count property in run 0 audit
Unable to locate glyph 4 pre-run property set in run 0 audit
   
   
Unable to locate glyph 5 name property in run 0 audit
Unable to locate glyph 5 version property in run 0 audit
Unable to locate glyph 5 input file count property in run 0 audit
Unable to locate glyph 5 input connection count property in run 0 audit
Unable to locate glyph 5 output connection count property in run 0 audit
Unable to locate glyph 5 pre-run property set in run 0 audit
   
   
Unable to locate glyph 6 name property in run 0 audit
Unable to locate glyph 6 version property in run 0 audit
Unable to locate glyph 6 input file count property in run 0 audit
Unable to locate glyph 6 input connection count property in run 0 audit
Unable to locate glyph 6 output connection count property in run 0 audit
Unable to locate glyph 6 pre-run property set in run 0 audit
   
   
Unable to locate glyph 7 name property in run 0 audit
Unable to locate glyph 7 version property in run 0 audit
Unable to locate glyph 7 input file count property in run 0 audit
Unable to locate glyph 7 input connection count property in run 0 audit
Unable to locate glyph 7 output connection count property in run 0 audit
Unable to locate glyph 7 pre-run property set in run 0 audit
   
   
Unable to locate glyph 8 name property in run 0 audit
Unable to locate glyph 8 version property in run 0 audit
Unable to locate glyph 8 input file count property in run 0 audit
Unable to locate glyph 8 input connection count property in run 0 audit
Unable to locate glyph 8 output connection count property in run 0 audit
Unable to locate glyph 8 pre-run property set in run 0 audit
   
   
Unable to locate glyph 9 name property in run 0 audit
Unable to locate glyph 9 version property in run 0 audit
Unable to locate glyph 9 input file count property in run 0 audit
Unable to locate glyph 9 input connection count property in run 0 audit
Unable to locate glyph 9 output connection count property in run 0 audit
Unable to locate glyph 9 pre-run property set in run 0 audit
   
   
Unable to locate glyph 10 name property in run 0 audit
Unable to locate glyph 10 version property in run 0 audit
Unable to locate glyph 10 input file count property in run 0 audit
Unable to locate glyph 10 input connection count property in run 0 audit
Unable to locate glyph 10 output connection count property in run 0 audit
Unable to locate glyph 10 pre-run property set in run 0 audit
   
   
Unable to locate glyph 11 name property in run 0 audit
Unable to locate glyph 11 version property in run 0 audit
Unable to locate glyph 11 input file count property in run 0 audit
Unable to locate glyph 11 input connection count property in run 0 audit
Unable to locate glyph 11 output connection count property in run 0 audit
Unable to locate glyph 11 pre-run property set in run 0 audit
   
   
Unable to locate glyph 12 name property in run 0 audit
Unable to locate glyph 12 version property in run 0 audit
Unable to locate glyph 12 input file count property in run 0 audit
Unable to locate glyph 12 input connection count property in run 0 audit
Unable to locate glyph 12 output connection count property in run 0 audit
Unable to locate glyph 12 pre-run property set in run 0 audit
   
   
Unable to locate glyph 13 name property in run 0 audit
Unable to locate glyph 13 version property in run 0 audit
Unable to locate glyph 13 input file count property in run 0 audit
Unable to locate glyph 13 input connection count property in run 0 audit
Unable to locate glyph 13 output connection count property in run 0 audit
Unable to locate glyph 13 pre-run property set in run 0 audit
   
   
Unable to locate glyph 14 name property in run 0 audit
Unable to locate glyph 14 version property in run 0 audit
Unable to locate glyph 14 input file count property in run 0 audit
Unable to locate glyph 14 input connection count property in run 0 audit
Unable to locate glyph 14 output connection count property in run 0 audit
Unable to locate glyph 14 pre-run property set in run 0 audit
   
   
Unable to locate glyph 15 name property in run 0 audit
Unable to locate glyph 15 version property in run 0 audit
Unable to locate glyph 15 input file count property in run 0 audit
Unable to locate glyph 15 input connection count property in run 0 audit
Unable to locate glyph 15 output connection count property in run 0 audit
Unable to locate glyph 15 pre-run property set in run 0 audit
   
   
Unable to locate glyph 16 name property in run 0 audit
Unable to locate glyph 16 version property in run 0 audit
Unable to locate glyph 16 input file count property in run 0 audit
Unable to locate glyph 16 input connection count property in run 0 audit
Unable to locate glyph 16 output connection count property in run 0 audit
Unable to locate glyph 16 pre-run property set in run 0 audit
   
   
   
   
   
In run audit data
   
   
Glyph 1 - "VibrationGenerator1"
   
Glyph 2 - "Bill_of_Materials_Input"
   
Glyph 3 - "Simulation_Input"
   
   
   
   
   
   
Post run audit data
   
Glyph 1 - "VibrationGenerator1"
   
Output channels - 1
Plugs - 1
Plug 1 - "Plug1"
Plug 1 pads - 1
Plug 1 pad 1 channels - 1
Plug 1, Pad 1, Channel 1 = Vibration Generator Channel (channel #1)
   
Properties - 19 entries (post-run state)
AdditionalNumberOfSweeps = 0
EndFrequency = 101
FrequencyStep = 1
InterpolationMethod = Log
Name = sine_sweep
NoiseFloor = -120
NumberOfBins = 1024
PSDUnits = Acceleration
SineAmplitudes = Undefined
SineFrequencies = Undefined
StartFrequency = 1
SweepRate = 1
SweepType = HZ/Sec (Linear)
TestDuration = 100
TestName = Undefined
TestType = Acceleration (g)
Type = SineSweep2
VibrationTable = PropertiesTab
XMLTables = <VibrationTables Version="1.0"><Tables><SineSweep/><SineDwell/><RandomPSD><RandomPSDItem Amplitude="1" Frequency="1"/><RandomPSDItem Amplitude="1" Frequency="1000"/></RandomPSD><SineOnRandom/><SineSweep2><SineSweep2Item Amplitude="0.1" Frequency="1"/><SineSweep2Item Amplitude="1" Frequency="10"/><SineSweep2Item Amplitude="1" Frequency="100"/></SineSweep2></Tables></VibrationTables>

   
Execution time - 0.0019283secs
   
   
Glyph 2 - "Bill_of_Materials_Input"
   
Output channels - 1
Plugs - 1
Plug 1 - "Plug1"
Plug 1 pads - 1
Plug 1 pad 1 channels - 1
Plug 1, Pad 1, Channel 1 =  (channel #1)
   
Properties - 7 entries (post-run state)
CombineAllTests = False
DiscardProcessedTests = False
LoopAllTests = True
MatchingMethod = ChannelNumber
SVDecimalSeparator = 
SVSeparator = 
SaveTestList = False
   
Execution time - 0.0165022secs
   
   
Glyph 3 - "Simulation_Input"
Plugs - 1
Plug 1 - "Plug1"
Plug 1 pads - 1
Plug 1 pad 1 channels - 0
   
Properties - 9 entries (post-run state)
CombineTests = True
DiscardProcessedTests = False
ImportUserGroups = False
LoadCaseNumbering = EachFile
LoadCases = Undefined
LoopAllTests = True
SaveTestList = False
StoreDisplayedGroups = False
UserGroupsFilename = Undefined
   
Execution time - 0.0001056secs
   
   
Unable to locate glyph 3 name property in run 0 audit
Unable to locate glyph 3 input channel count property in run 0 audit
Unable to locate glyph 3 socket count property in run 0 audit
Unable to locate glyph 3 output channel count property in run 0 audit
Unable to locate glyph 3 plug count property in run 0 audit
Unable to locate glyph 3 output file count property in run 0 audit
Unable to locate glyph 3 post-run property set in run 0 audit
   
Unable to locate glyph 3 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 4 name property in run 0 audit
Unable to locate glyph 4 input channel count property in run 0 audit
Unable to locate glyph 4 socket count property in run 0 audit
Unable to locate glyph 4 output channel count property in run 0 audit
Unable to locate glyph 4 plug count property in run 0 audit
Unable to locate glyph 4 output file count property in run 0 audit
Unable to locate glyph 4 post-run property set in run 0 audit
   
Unable to locate glyph 4 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 5 name property in run 0 audit
Unable to locate glyph 5 input channel count property in run 0 audit
Unable to locate glyph 5 socket count property in run 0 audit
Unable to locate glyph 5 output channel count property in run 0 audit
Unable to locate glyph 5 plug count property in run 0 audit
Unable to locate glyph 5 output file count property in run 0 audit
Unable to locate glyph 5 post-run property set in run 0 audit
   
Unable to locate glyph 5 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 6 name property in run 0 audit
Unable to locate glyph 6 input channel count property in run 0 audit
Unable to locate glyph 6 socket count property in run 0 audit
Unable to locate glyph 6 output channel count property in run 0 audit
Unable to locate glyph 6 plug count property in run 0 audit
Unable to locate glyph 6 output file count property in run 0 audit
Unable to locate glyph 6 post-run property set in run 0 audit
   
Unable to locate glyph 6 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 7 name property in run 0 audit
Unable to locate glyph 7 input channel count property in run 0 audit
Unable to locate glyph 7 socket count property in run 0 audit
Unable to locate glyph 7 output channel count property in run 0 audit
Unable to locate glyph 7 plug count property in run 0 audit
Unable to locate glyph 7 output file count property in run 0 audit
Unable to locate glyph 7 post-run property set in run 0 audit
   
Unable to locate glyph 7 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 8 name property in run 0 audit
Unable to locate glyph 8 input channel count property in run 0 audit
Unable to locate glyph 8 socket count property in run 0 audit
Unable to locate glyph 8 output channel count property in run 0 audit
Unable to locate glyph 8 plug count property in run 0 audit
Unable to locate glyph 8 output file count property in run 0 audit
Unable to locate glyph 8 post-run property set in run 0 audit
   
Unable to locate glyph 8 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 9 name property in run 0 audit
Unable to locate glyph 9 input channel count property in run 0 audit
Unable to locate glyph 9 socket count property in run 0 audit
Unable to locate glyph 9 output channel count property in run 0 audit
Unable to locate glyph 9 plug count property in run 0 audit
Unable to locate glyph 9 output file count property in run 0 audit
Unable to locate glyph 9 post-run property set in run 0 audit
   
Unable to locate glyph 9 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 10 name property in run 0 audit
Unable to locate glyph 10 input channel count property in run 0 audit
Unable to locate glyph 10 socket count property in run 0 audit
Unable to locate glyph 10 output channel count property in run 0 audit
Unable to locate glyph 10 plug count property in run 0 audit
Unable to locate glyph 10 output file count property in run 0 audit
Unable to locate glyph 10 post-run property set in run 0 audit
   
Unable to locate glyph 10 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 11 name property in run 0 audit
Unable to locate glyph 11 input channel count property in run 0 audit
Unable to locate glyph 11 socket count property in run 0 audit
Unable to locate glyph 11 output channel count property in run 0 audit
Unable to locate glyph 11 plug count property in run 0 audit
Unable to locate glyph 11 output file count property in run 0 audit
Unable to locate glyph 11 post-run property set in run 0 audit
   
Unable to locate glyph 11 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 12 name property in run 0 audit
Unable to locate glyph 12 input channel count property in run 0 audit
Unable to locate glyph 12 socket count property in run 0 audit
Unable to locate glyph 12 output channel count property in run 0 audit
Unable to locate glyph 12 plug count property in run 0 audit
Unable to locate glyph 12 output file count property in run 0 audit
Unable to locate glyph 12 post-run property set in run 0 audit
   
Unable to locate glyph 12 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 13 name property in run 0 audit
Unable to locate glyph 13 input channel count property in run 0 audit
Unable to locate glyph 13 socket count property in run 0 audit
Unable to locate glyph 13 output channel count property in run 0 audit
Unable to locate glyph 13 plug count property in run 0 audit
Unable to locate glyph 13 output file count property in run 0 audit
Unable to locate glyph 13 post-run property set in run 0 audit
   
Unable to locate glyph 13 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 14 name property in run 0 audit
Unable to locate glyph 14 input channel count property in run 0 audit
Unable to locate glyph 14 socket count property in run 0 audit
Unable to locate glyph 14 output channel count property in run 0 audit
Unable to locate glyph 14 plug count property in run 0 audit
Unable to locate glyph 14 output file count property in run 0 audit
Unable to locate glyph 14 post-run property set in run 0 audit
   
Unable to locate glyph 14 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 15 name property in run 0 audit
Unable to locate glyph 15 input channel count property in run 0 audit
Unable to locate glyph 15 socket count property in run 0 audit
Unable to locate glyph 15 output channel count property in run 0 audit
Unable to locate glyph 15 plug count property in run 0 audit
Unable to locate glyph 15 output file count property in run 0 audit
Unable to locate glyph 15 post-run property set in run 0 audit
   
Unable to locate glyph 15 post-run execution time property in run 0 audit
   
   
Unable to locate glyph 16 name property in run 0 audit
Unable to locate glyph 16 input channel count property in run 0 audit
Unable to locate glyph 16 socket count property in run 0 audit
Unable to locate glyph 16 output channel count property in run 0 audit
Unable to locate glyph 16 plug count property in run 0 audit
Unable to locate glyph 16 output file count property in run 0 audit
Unable to locate glyph 16 post-run property set in run 0 audit
   
Unable to locate glyph 16 post-run execution time property in run 0 audit
   
   
Single run - PASSED
End time - 15-Aug-2025 15:15:56
   
   
   
Product         GlyphWorks V25.0.0 Release Build 431
Platform        Windows64
abcdlib         V25.0 A01 Jan 14 2025 12:42:50
ailib           V25.0 A01 Jan 14 2025 12:43:34
Ans.DesignLifeAddin V25.1 A00 Tuesday, January 14, 2025 1:48:14 PM
anslib          V25.0 A01 Jan 14 2025 12:43:19
asamlib         V25.0 A01 Jan 14 2025 13:07:33
atlib           V25.0 A01 Jan 14 2025 12:51:03
CBLib           V25.0 A01 Jan 14 2025 12:43:46
cgdlib          V25.0 A01 Jan 14 2025 12:48:23
cgflib          V25.0 A01 Jan 14 2025 12:41:16
cgolib          V25.0 A01 Jan 14 2025 12:48:07
cgrlib          V25.0 A01 Jan 14 2025 12:47:43
cpputil         V25.0 A01 Jan 14 2025 12:34:31
dglib           V25.0 A01 Jan 14 2025 12:50:00
dmilib          V25.0 A01 Jan 14 2025 12:35:37
dtlib           V25.0 A01 Jan 14 2025 12:47:07
extlib          V25.0 A01 Jan 14 2025 12:32:12
fatlib          V25.0 A01 Jan 14 2025 12:39:41
FDLib           V25.0 A01 Jan 14 2025 12:44:23
fedlib          V25.0 A01 Jan 14 2025 12:53:52
feilib          V25.0 A01 Jan 14 2025 12:43:08
feimportlib (ANSYS) V25.0 A01 Jan 14 2025 12:46:38
ferlib          V25.0 A01 Jan 14 2025 12:37:58
fiolib          V25.0 A01 Jan 14 2025 12:42:00
FSLib           V25.0 A01 Jan 14 2025 12:37:05
FVLib           V25.0 A01 Jan 14 2025 12:56:58
GlyphEngine01   V25.0 A01 Jan 14 2025 12:59:10
GlyphEngine02   V25.0 A01 Jan 14 2025 12:59:49
GlyphEngine03   V25.0 A01 Jan 14 2025 13:00:38
GlyphEngine04   V25.0 A01 Jan 14 2025 13:01:39
GlyphEngine06   V25.0 A01 Jan 14 2025 13:02:36
GlyphEngine07   V25.0 A01 Jan 14 2025 13:03:02
GlyphEngine08   V25.0 A01 Jan 14 2025 13:03:23
GlyphEngine09   V25.0 A01 Jan 14 2025 13:03:48
GlyphEngine10   V25.0 A01 Jan 14 2025 13:04:14
GlyphEngine13   V25.0 A01 Jan 14 2025 13:04:39
GlyphEngine14   V25.0 A01 Jan 14 2025 13:05:28
GlyphEngine15   V25.0 A01 Jan 14 2025 13:05:56
GlyphEngine16   V25.0 A01 Jan 14 2025 13:06:24
grlib           V25.0 A01 Jan 14 2025 12:51:53
gutlib          V25.0 A01 Jan 14 2025 12:55:50
iceintlib       V25.0 A01 Jan 14 2025 12:50:33
IXDLib          V25.0 A01 Jan 14 2025 12:35:52
jprolib         V25.0 A01 Jan 14 2025 12:42:35
lican           V25.0 A01 Jan 14 2025 12:30:34
licnc           V25.0 A01 Jan 14 2025 12:30:19
licsh           V25.0 A01 Jan 14 2025 12:30:10
maplib          V25.0 A01 Jan 14 2025 12:35:25
matdblib        V25.0 A01 Jan 14 2025 12:38:15
materials       V25.0 A01 Jan 14 2025 12:49:26
mcxlib          V25.0 A01 Jan 14 2025 12:32:51
mthlib          V25.0 A01 Jan 14 2025 12:35:14
mtlib           V25.0 A01 Jan 14 2025 12:33:48
ncmpilib        V25.0 A01 Jan 14 2025 12:32:18
ncodedesktop    V25.0 A01 Jan 14 2025 13:27:32
ncxml           V25.0 A01 Jan 14 2025 12:30:42
nmxfiolib       V25.0 A01 Jan 14 2025 12:37:45
nulib           V25.0 A01 Jan 14 2025 12:34:46
NXLib           V25.0 A01 Jan 14 2025 12:33:01
PipeData00      V25.0 A01 Jan 14 2025 12:55:01
ProgramEngine00 V25.0 A01 Jan 14 2025 13:06:46
pylib           V25.0 A01 Jan 14 2025 12:33:57
QCLib           V25.0 A01 Jan 14 2025 12:55:21
qtutil          V25.0 A01 Jan 14 2025 12:48:50
QXLib           V25.0 A01 Jan 14 2025 12:45:08
S3Lib           V25.0 A01 Jan 14 2025 12:33:22
sielib          V25.0 A01 Jan 14 2025 12:37:35
siglib          V25.0 A01 Jan 14 2025 12:40:54
utlib (ANSYS)   V25.0 A01 Jan 14 2025 12:28:47
xllib           V25.0 A01 Jan 14 2025 12:31:01
Pre run audit data
   
Start time - 15-Aug-2025 15:16:15
Single run
Flow file - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-2\DL\dl.fdb
Glyph count - 17
   
   
Glyph 1 - "VibrationGenerator1"
Version - 5
   
Output connections - 1
Output connection 1:1 - Plug1.Vibration Profile to SweptSine_Analysis.Histogram.HistogramPipe1
Output connection 1:2 - Plug1.Vibration Profile to Swept Sine Display.HistSocket.s1b
   
Properties - 19 entries (pre-run state)
AdditionalNumberOfSweeps = 0
EndFrequency = 101
FrequencyStep = 1
InterpolationMethod = Log
Name = sine_sweep
NoiseFloor = -120
NumberOfBins = 1024
PSDUnits = Acceleration
SineAmplitudes = Undefined
SineFrequencies = Undefined
StartFrequency = 1
SweepRate = 1
SweepType = HZ/Sec (Linear)
TestDuration = 100
TestName = Undefined
TestType = Acceleration (g)
Type = SineSweep2
VibrationTable = PropertiesTab
XMLTables = <VibrationTables Version="1.0"><Tables><SineSweep/><SineDwell/><RandomPSD><RandomPSDItem Amplitude="1" Frequency="1"/><RandomPSDItem Amplitude="1" Frequency="1000"/></RandomPSD><SineOnRandom/><SineSweep2><SineSweep2Item Amplitude="0.1" Frequency="1"/><SineSweep2Item Amplitude="1" Frequency="10"/><SineSweep2Item Amplitude="1" Frequency="100"/></SineSweep2></Tables></VibrationTables>

   
   
Glyph 2 - "Bill_of_Materials_Input"
Version - 7
   
Input files - 1
Input file 1 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-2\DL\dlbom.csv;amc;c1
   
Output connections - 1
Output connection 1:1 - Plug1.P1a to SweptSine_Analysis.MaterialMapLoader.Use materials from Workbench
   
Properties - 7 entries (pre-run state)
CombineAllTests = False
DiscardProcessedTests = False
LoopAllTests = True
MatchingMethod = ChannelNumber
SVDecimalSeparator = 
SVSeparator = 
SaveTestList = False
   
   
Glyph 3 - "Simulation_Input"
Version - 8
   
Input files - 2
Input file 1 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\MECH\file.rst;afe;c1
Input file 2 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-1\MECH\file.rst;afe;c1
   
Output connections - 1
Output connection 1:1 - Plug1.FE Model Data to SweptSine_Analysis.FEMetaData.FRF Input
Output connection 1:2 - Plug1.FE Model Data to SweptSine_Analysis.FEMetaData.Offset Loadcase Input
   
Properties - 9 entries (pre-run state)
CombineTests = True
DiscardProcessedTests = False
ImportUserGroups = False
LoadCaseNumbering = EachFile
LoadCases = Undefined
LoopAllTests = True
SaveTestList = False
StoreDisplayedGroups = False
UserGroupsFilename = Undefined
   
   
Glyph 4 - "SweptSine_Analysis"
Version - 8
   
Input connections - 4
Input connection 1 - FEMetaData.FRF Input from Simulation_Input.Plug1.FE Model Data
Input connection 2 - FEMetaData.Offset Loadcase Input from Simulation_Input.Plug1.FE Model Data
Input connection 3 - MaterialMapLoader.Use materials from Workbench from Bill_of_Materials_Input.Plug1.P1a
Input connection 4 - Histogram.HistogramPipe1 from VibrationGenerator1.Plug1.Vibration Profile
   
Output connections - 4
Output connection 1:1 - Results.Compressed results (for display) to HotSpotDetection1.CAE Fatigue Results.CAE Fatigue Results
Output connection 1:2 - Results.Compressed results (for display) to FER_File_Output.S1.S1a
Output connection 1:3 - Results.Compressed results (for display) to Fatigue_Results_Display.FE Results.FE Results
Output connection 1:4 - Results.Compressed results (for display) to MultiColumnFilter1.Socket1.Multi-Column Input
Output connection 1:5 - Results.Compressed results (for display) to DataValuesDisplay.S1.S1c
Output connection 1:6 - Results.Compressed results (for display) to Design Explorer Output1.Linked to SGInput1.Input 1
Output connection 2:1 - MultiColumn.PSD of Stress to Stress_Amplitude_Spectrum.MCSocket.Multi-Column Input 1
Output connection 3:1 - Histogram.Cycles Histogram to Cycles_Histogram.S1.Histogram Input 1
Output connection 4:1 - Histogram.Damage Histogram to Damage_Histogram.S1.Histogram Input 1
   
Properties - 23 entries (pre-run state)
AnalysisGroup_GroupNames = *
AnalysisGroup_MaterialAssignmentGroup = Material
AnalysisGroup_SelectionGroupType = FEInput
AnalysisGroup_ShellLayer = TopAndBottom
AnalysisGroup_SolutionLocation = AveragedNodeOnElement
AnalysisGroup_UnitsDefinition = MPA,MM,N,TNMM,DEGC
Job_NumAnalysisThreads = ?
LogMessageLimit = 100
LoggingLevel = Info
ResultsUpdateInterval = 10
SNEngine_CertaintyOfSurvival = 50
SNEngine_CombinationMethod = AbsMaxPrincipal
SNEngine_MeanStressCorrection = Interpolate
SNEngine_SNMethod = MultiRRatioCurve
Use materials from Workbench_Active = True
VibrationLoad_FrequencySelectionMethod = FRFFrequencies
VibrationLoad_InterpolationMethod = LogLog
VibrationLoad_LoadingMethod = SineSweep
VibrationLoad_SineDwellDurationSeconds = 600
VibrationLoad_SineDwellFrequency = 10
VibrationLoad_SweepRate = 1
VibrationLoad_SweepType = LinearHzPerSec
matml_DatabaseName = C:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\ENGD\material.engd
   
   
Glyph 5 - "HotSpotDetection1"
Version - 3
   
Input connections - 1
Input connection 1 - CAE Fatigue Results.CAE Fatigue Results from SweptSine_Analysis.Results.Compressed results (for display)
   
Output connections - 1
Output connection 1:1 - Hot Spot List.Hot Spot List to HotSpot_List_Output.Socket1.S1a
Output connection 1:2 - Hot Spot List.Hot Spot List to Fatigue_Results_Display.Feature List.Hot Spot List
   
Properties - 9 entries (pre-run state)
CategoryColumnKeyword = Undefined
ColumnsToOutput = Undefined
EntityType = Auto
HotSpotDataKeyword = Damage
HotSpotPeakDirection = Max
IncludeAdjacentLocations = False
MaxNumCategories = 100
MaxNumHotSpots = 10
ProcessByCategory = False
   
   
Glyph 6 - "FER_File_Output"
Version - 8
   
Input connections - 1
Input connection 1 - S1.S1a from SweptSine_Analysis.Results.Compressed results (for display)
   
Properties - 21 entries (pre-run state)
CategoryKeepCount = 1
CategoryKeyword = Undefined
CompressResults = True
EquivUnits = Repeats
EventNaming = Name
ExportCSVDecimalSeparator = 
ExportCSVSeparator = 
GroupType = Property
IncludeSolids = True
MaxGroups = 1000
MinersSum = 1
MultipleEventsSingleODB = False
NodeOnElementCompression = Element
NumEquivUnits = 1
ODBInputFilename = Undefined
OutputFilename = #Test.InputTestInfo.TestName#
OutputFormat = nCode_FER
Overwrite = Yes
Record4ConfigFile = 
ShellLayer = Worst
SortKeywords = -damage
   
   
Glyph 7 - "HotSpot_List_Output"
Version - 4
   
Input connections - 1
Input connection 1 - Socket1.S1a from HotSpotDetection1.Hot Spot List.Hot Spot List
   
Properties - 13 entries (pre-run state)
ASAMDataModel = Undefined
AddToFileList = False
ClearInputGlyphFiles = True
EnumOutput = String
ExportSVDecimalSeparator = 
ExportSVSeparator = 
FileFormat = S3MultiColumn
LoadOutputFilesIntoInputGlyph = 
MetaDataOutput = SaveWithTest
NameText = HotSpot_List
NamingMethod = NewName
Overwrite = Yes
WriteMetadataToSV = False
   
   
Glyph 8 - "Fatigue_Results_Display"
Version - 2
   
Input connections - 2
Input connection 1 - FE Results.FE Results from SweptSine_Analysis.Results.Compressed results (for display)
Input connection 2 - Feature List.Hot Spot List from HotSpotDetection1.Hot Spot List.Hot Spot List
   
Properties - 1 entries (pre-run state)
ModelFilename = 
   
   
Glyph 9 - "Swept Sine Display"
Version - 1
   
Input connections - 1
Input connection 1 - HistSocket.s1b from VibrationGenerator1.Plug1.Vibration Profile
   
Properties - 30 entries (pre-run state)
CursorOutput = None
CursorReceive = None
CursorSend = None
HarmonicXCursors = None
LegendHeightPercent = 25
NameTextInput1 = _in1
NameTextInput2 = _in2
NameTextInput3 = _in3
NameTextInput4 = _in4
NameTextInput5 = _in5
NameTextInput6 = _in6
NameTextInput7 = _in7
NameTextInput8 = _in8
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
NamingMethodInput3 = Suffix
NamingMethodInput4 = Suffix
NamingMethodInput5 = Suffix
NamingMethodInput6 = Suffix
NamingMethodInput7 = Suffix
NamingMethodInput8 = Suffix
NumHistogramInputPads = 2
NumMultiColumnInputPads = 2
NumTsInputPads = 2
NumberPeakCursors = 3
PeakXcursors = None
ShowLegend = False
StoreCursors = False
XCursors = 
YCursors = 
   
   
Glyph 10 - "Cycles_Histogram"
Version - 1
   
Input connections - 1
Input connection 1 - S1.Histogram Input 1 from SweptSine_Analysis.Histogram.Cycles Histogram
   
Properties - 4 entries (pre-run state)
NameTextInput1 = _in1
NameTextInput2 = _in2
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
   
   
Glyph 11 - "Stress_Amplitude_Spectrum"
Version - 1
   
Input connections - 1
Input connection 1 - MCSocket.Multi-Column Input 1 from SweptSine_Analysis.MultiColumn.PSD of Stress
   
Properties - 30 entries (pre-run state)
CursorOutput = None
CursorReceive = CursorA
CursorSend = CursorA
HarmonicXCursors = None
LegendHeightPercent = 25
NameTextInput1 = _in1
NameTextInput2 = _in2
NameTextInput3 = _in3
NameTextInput4 = _in4
NameTextInput5 = _in5
NameTextInput6 = _in6
NameTextInput7 = _in7
NameTextInput8 = _in8
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
NamingMethodInput3 = Suffix
NamingMethodInput4 = Suffix
NamingMethodInput5 = Suffix
NamingMethodInput6 = Suffix
NamingMethodInput7 = Suffix
NamingMethodInput8 = Suffix
NumHistogramInputPads = 2
NumMultiColumnInputPads = 2
NumTsInputPads = 2
NumberPeakCursors = 3
PeakXcursors = None
ShowLegend = False
StoreCursors = True
XCursors = Undefined
YCursors = Undefined
   
   
Glyph 12 - "Damage_Histogram"
Version - 1
   
Input connections - 1
Input connection 1 - S1.Histogram Input 1 from SweptSine_Analysis.Histogram.Damage Histogram
   
Properties - 4 entries (pre-run state)
NameTextInput1 = _in1
NameTextInput2 = _in2
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
   
   
Glyph 13 - "MultiColumnFilter1"
Version - 1
   
Input connections - 1
Input connection 1 - Socket1.Multi-Column Input from SweptSine_Analysis.Results.Compressed results (for display)
   
Output connections - 1
Output connection 1:1 - Plug1.Multi-Column Output to CSV_File_Output.S1.S1a
   
Properties - 7 entries (pre-run state)
Channels = Undefined
ColumnsToExclude = Undefined
ColumnsToInclude = NodeID,Damage,Life
FilterCaseSensitive = False
FilterColumn = Undefined
FilterComparison = =
FilterValue = Undefined
   
   
Glyph 14 - "CSV_File_Output"
Version - 8
   
Input connections - 1
Input connection 1 - S1.S1a from MultiColumnFilter1.Plug1.Multi-Column Output
   
Properties - 21 entries (pre-run state)
CategoryKeepCount = 1
CategoryKeyword = Undefined
CompressResults = True
EquivUnits = Repeats
EventNaming = Name
ExportCSVDecimalSeparator = 
ExportCSVSeparator = 
GroupType = Property
IncludeSolids = True
MaxGroups = 1000
MinersSum = 1
MultipleEventsSingleODB = False
NodeOnElementCompression = Element
NumEquivUnits = 1
ODBInputFilename = Undefined
OutputFilename = dl_results
OutputFormat = CSV
Overwrite = Yes
Record4ConfigFile = 
ShellLayer = Worst
SortKeywords = -damage
   
   
Glyph 15 - "DX_parameters"
Version - 1
   
Output connections - 1
Output connection 1:1 - Output.Metadata Output to Design Explorer Output1.Linked to SGInput1.Metadata Input
   
Properties - 4 entries (pre-run state)
HideSetupTabs = True
Parameter_per_group = False
Parameter_type = life
Properties = <Properties><Property help="If True, a parameter for each material group is exported. If False a single parameter for the entire model is exported." name="Parameter_per_group" type="boolean" mandatory="true" description="Export a parameter for each material group, or a single parameter for the model"/><Property help="The worst result of this type will be passed back to DesignExplorer. Fatigue analyses for damage can export either life or damage. Backcalculation analyses can export scalefactor, and DangVan can export safetyfactor. On a dutycycle run, the total schedule results is used." name="Parameter_type" type="enum" enumopts="damage,life,safetyfactor,scalefactor" mandatory="true" description="Type of fatigue result to pass to DesignExplorer"/></Properties>
   
   
Glyph 16 - "Design Explorer Output1"
Version - 1
   
Input connections - 2
Input connection 1 - Linked to SGInput1.Input 1 from SweptSine_Analysis.Results.Compressed results (for display)
Input connection 2 - Linked to SGInput1.Metadata Input from DX_parameters.Output.Metadata Output
   
Properties - 5 entries (pre-run state)
BitmapFileName = SuperGlyph
IconFileName = SuperGlyph
Locked = False
Verbose = True
   
   
Glyph 17 - "DataValuesDisplay"
Version - 13
   
Input connections - 1
Input connection 1 - S1.S1c from SweptSine_Analysis.Results.Compressed results (for display)
   
Properties - 33 entries (pre-run state)
2DHistogramVerticalFormat = True
ChannelsToDisplay = Undefined
ColumnLabel = AxisTitle
Columns = 
ColumnsToColour = 
DisplayMode = Mag/Phase
EqualsColour = LightGreen
EqualsTolerance = 1E-4
EqualsValue = ?
ExportCSVDecimalSeparator = 
ExportCSVSeparator = 
ExportNameText = Undefined
ExportNamingMethod = Suffix
ExportType = None
HistogramBinLabels = BinCentre
IntegerFormat = Decimal
IntervalUnits = Point
LowerGate = ?
LowerGateColour = Blue
MaximumValueColour = Undefined
MinimumValueColour = Undefined
MissingValuesSpace = True
NumberSigFig = 4
Overwrite = Ask
PointIncrementValue = 10
ReverseYAxis = False
ShowColumnKeywords = False
ShowColumnTypes = False
TransposeXY = Normal
UTCFormat = Local
UpperGate = ?
UpperGateColour = Red
XAxisUnitsIncrementValue = 1
   
   
   
   
   
In run audit data
   
   
Glyph 1 - "VibrationGenerator1"
   
Glyph 2 - "Bill_of_Materials_Input"
   
Glyph 3 - "Simulation_Input"
   
Glyph 4 - "SweptSine_Analysis"
   
Glyph 5 - "HotSpotDetection1"
   
Glyph 6 - "FER_File_Output"
   
Glyph 7 - "HotSpot_List_Output"
   
Glyph 8 - "Fatigue_Results_Display"
   
Glyph 9 - "Swept Sine Display"
   
Glyph 10 - "Cycles_Histogram"
   
Glyph 11 - "Stress_Amplitude_Spectrum"
   
Glyph 12 - "Damage_Histogram"
   
Glyph 13 - "MultiColumnFilter1"
   
Glyph 14 - "CSV_File_Output"
   
Glyph 15 - "DX_parameters"
   
Glyph 16 - "Design Explorer Output1"
2 info messages
Info 1 - . > Design Explorer Output1 (n=1)
Info 2 - . < Design Explorer Output1 (n=1) 0.3749secs
   
Glyph 17 - "DataValuesDisplay"
   
   
   
   
"Job" - 7 entries
"AuditFilename" = Undefined
"Description" = 
"IgnoreUnusedArguments" = False
"MemoryLogging" = False
"NumAnalysisThreads" = ?
"OverwriteAuditFile" = Append
"ValidateAutoConfigureLoading" = Warn
   
"SweptSine_Analysis" - 1 entries
"CAEConfiguration" = 
OBJECT ** Job ** (DTJob : Job)
{
  AuditFilename=<Not set>
  Description=
  IgnoreUnusedArguments=False
  MemoryLogging=False
  NumAnalysisThreads=<Not set>
  OverwriteAuditFile=Append
  ValidateAutoConfigureLoading=Warn
  CHILDREN of Job
  {
    OBJECT ** Run1 ** (DTRun : Run)
    {
      Gate=20
      GateUnits=Percent
      NumAnalysisThreads=<Not set>
      TimeHistoryCompression=None
      ATTACHMENTS to Run1
      {
        OBJECT ** AnaDef ** (DTAnalysisDefinition : Analysis definition)
        {
          AnalysisGroups=*
          AutoEliminationMode=False
          CompressionOverride=SameAsRun
          EntitySubsetCombination=<Not set>
          Gate=0
          GateUnits=Percent
          ATTACHMENTS to AnaDef
          {
            OBJECT ** SNEngine ** (DTAnalysisEngineSN : Standard SN analysis engine)
            {
              AngleInterval=10
              BackCalcAccuracy=1
              BackCalcMaxScale=5
              BackCalcMinScale=0.2
              BackCalcMode=None
              BiaxialityGate=20
              BiaxialityThresholdLower=-0.6
              BiaxialityThresholdUpper=0.6
              CertaintyOfSurvival=50
              CheckStaticFailure=False
              CombinationMethod=AbsMaxPrincipal
              CompressByMaxStress=False
              CustomSNMethod=CustomSNTest
              DamageFloor=1E-15
              EventProcessing=Independent
              FatigueReserveFactor=1
              InterpolationLimit=UseMaxCurve
              MaxDamage=1E30
              MeanStressCorrection=Interpolate
              MeanStressCorrectionStrengthParameter=YieldStrength
              MeanStressExponent=1
              MultiAxialAssessment=None
              NonPropFactorThreshold=0.25
              OutputDistributedSource=False
              OutputEventResults=False
              OutputMaterialNames=False
              OutputMaxMin=False
              OutputStats=False
              OutputStressGradientFactors=False
              OutputVibrationStats=False
              SNMethod=MultiRRatioCurve
              ScaleFactor=1
              ScaleNormalStress=False
              SmallCycleCorrection=None
              StaticFailureDamage=2
              StressGradientMethod=VonMises
              StressGradients=Auto
              StressGradientsUser=<Not set>
              TargetDamage=1E-6
              TemperatureInterpolationLimit=UseMaxCurve
              TemperatureSelection=CycleMax
              ZeroCompressiveDamage=Off
              ZeroDamageStressPercent=10
            }
            OBJECT ** MaterialMap ** (DTMaterialMap : Material map)
            {
              CSVFilename=
              DataSetType=nCodeSNRRatioCurveContainer
              DatabaseName=matml
              HideInternalMaterials=True
              MaterialSource=Database
              Permissions=Editable
              SaveMapping=True
              ValidateBeforeRun=False
              WeldLookupFilename=
              CHILDREN of MaterialMap
              {
                OBJECT ** Use materials from Workbench ** (DTMaterialMapLoaderPipe : Material map loader from pipe)
                {
                  Active=True
                  AdditionalDataKeys=Part,Material
                  ClearMap=True
                  MapEntryProperties=
                  MaterialGroupNameKeys=MaterialGroup
                  MaterialNameKey=Material
                }
                OBJECT ** MAT_1 ** (DTMaterialMapEntry : Material map entry)
                {
                  AdhesiveThickness=0.1
                  BondDistanceUnits=mm
                  BondLineOffset=0
                  CutEdgeLocation=None
                  DangVanParameterFilename=<Not set>
                  DatabaseName=<Not set>
                  DefaultMaterial=False
                  DefaultTemperature=0
                  InitialCrackSize=0.4
                  KRoughness=1
                  KTreatment=1
                  KUser=1
                  Material=Test_mat
                  ScaleFactor=1
                  ShapeFactor=<Not set>
                  StressOffset=0
                  StressOffsetUnits=MPa
                  SurfaceRoughness=0
                  SurfaceRoughnessType=Polished
                  WeldDiameter=<Not set>
                  WeldDiameterMethod=Auto
                  WeldDiameterUnits=mm
                  WeldLookupFilename=<Not set>
                }
                OBJECT ** MAT_2 ** (DTMaterialMapEntry : Material map entry)
                {
                  AdhesiveThickness=0.1
                  BondDistanceUnits=mm
                  BondLineOffset=0
                  CutEdgeLocation=None
                  DangVanParameterFilename=<Not set>
                  DatabaseName=<Not set>
                  DefaultMaterial=False
                  DefaultTemperature=0
                  InitialCrackSize=0.4
                  KRoughness=1
                  KTreatment=1
                  KUser=1
                  Material=Test_mat
                  ScaleFactor=1
                  ShapeFactor=<Not set>
                  StressOffset=0
                  StressOffsetUnits=MPa
                  SurfaceRoughness=0
                  SurfaceRoughnessType=Polished
                  WeldDiameter=<Not set>
                  WeldDiameterMethod=Auto
                  WeldDiameterUnits=mm
                  WeldLookupFilename=<Not set>
                }
              }
            }
            OBJECT ** PostProcessorElimination1 ** (DTPostProcessorElimination : Elimination post processor)
            {
              CategoryKeyword=<Not set>
              ColumnsToOutput=
              CountToKeep=1
              EntitySubsetName=gage
              HotSpotPeakDirection=Max
              IncludeAdjacentLocations=False
              KeepMode=Auto
              Limit=<Not set>
              LowerLimit=<Not set>
              MaxNumCategories=100
              MaxNumHotSpots=5
              Mode=HighestCount
              PercentToKeep=10
              ResultKeyword=Damage
              SecondaryFilter=None
              SecondaryLimit=<Not set>
              UpperLimit=<Not set>
            }
          }
        }
      }
    }
    OBJECT ** matml ** (DTMaterialDatabasenCode : nCode material database)
    {
      DatabaseName=C:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\ENGD\material.engd
      DatabaseType=MML
    }
    OBJECT ** Run2 ** (DTRun : Run)
    {
      Gate=0
      GateUnits=Percent
      NumAnalysisThreads=<Not set>
      TimeHistoryCompression=None
      ATTACHMENTS to Run2
      {
        OBJECT ** AnalysisDefinition1 ** (DTAnalysisDefinition : Analysis definition)
        {
          AnalysisGroups=*
          AutoEliminationMode=False
          CompressionOverride=SameAsRun
          EntitySubsetCombination=<Not set>
          Gate=0
          GateUnits=Percent
          ATTACHMENTS to AnalysisDefinition1
          {
            OBJECT ** AnalysisEngineSN1 ** (DTAnalysisEngineSN : Standard SN analysis engine)
            {
              AngleInterval=10
              BackCalcAccuracy=1
              BackCalcMaxScale=5
              BackCalcMinScale=0.2
              BackCalcMode=None
              BiaxialityGate=20
              BiaxialityThresholdLower=-0.6
              BiaxialityThresholdUpper=0.6
              CertaintyOfSurvival=50
              CheckStaticFailure=False
              CombinationMethod=AbsMaxPrincipal
              CompressByMaxStress=False
              CustomSNMethod=None
              DamageFloor=0
              EventProcessing=Independent
              FatigueReserveFactor=1
              InterpolationLimit=UseMaxCurve
              MaxDamage=0
              MeanStressCorrection=Interpolate
              MeanStressCorrectionStrengthParameter=YieldStrength
              MeanStressExponent=1
              MultiAxialAssessment=None
              NonPropFactorThreshold=0.25
              OutputDistributedSource=False
              OutputEventResults=False
              OutputMaterialNames=False
              OutputMaxMin=False
              OutputStats=False
              OutputStressGradientFactors=False
              OutputVibrationStats=False
              SNMethod=MultiRRatioCurve
              ScaleFactor=1
              ScaleNormalStress=False
              SmallCycleCorrection=None
              StaticFailureDamage=2
              StressGradientMethod=VonMises
              StressGradients=Auto
              StressGradientsUser=<Not set>
              TargetDamage=1E-6
              TemperatureInterpolationLimit=UseMaxCurve
              TemperatureSelection=CycleMax
              ZeroCompressiveDamage=Off
              ZeroDamageStressPercent=0
              ATTACHMENTS to AnalysisEngineSN1
              {
                OBJECT ** VibrationPSDOutput1 ** (DTVibrationPSDOutput : Vibration PSD output)
                {
                  ATTACHMENTS to VibrationPSDOutput1
                  {
                    OBJECT ** PSD of Stress ** (DTMultiColumnOutputPipe : Multi-column output to pipe)
                    {
                    }
                  }
                }
                OBJECT ** Cycles Histogram ** (DTHistogramOutputPipe : Histogram output to pipe)
                {
                  HistogramType=Rainflow
                }
                OBJECT ** Damage Histogram ** (DTHistogramOutputPipe : Histogram output to pipe)
                {
                  HistogramType=Damage
                }
              }
            }
            OBJECT ** MaterialMap ** (DTMaterialMap : Material map)
            {
              CSVFilename=
              DataSetType=nCodeSNRRatioCurveContainer
              DatabaseName=matml
              HideInternalMaterials=True
              MaterialSource=Database
              Permissions=Editable
              SaveMapping=True
              ValidateBeforeRun=False
              WeldLookupFilename=
              CHILDREN of MaterialMap
              {
                OBJECT ** Use materials from Workbench ** (DTMaterialMapLoaderPipe : Material map loader from pipe)
                {
                  Active=True
                  AdditionalDataKeys=Part,Material
                  ClearMap=True
                  MapEntryProperties=
                  MaterialGroupNameKeys=MaterialGroup
                  MaterialNameKey=Material
                }
                OBJECT ** MAT_1 ** (DTMaterialMapEntry : Material map entry)
                {
                  AdhesiveThickness=0.1
                  BondDistanceUnits=mm
                  BondLineOffset=0
                  CutEdgeLocation=None
                  DangVanParameterFilename=<Not set>
                  DatabaseName=<Not set>
                  DefaultMaterial=False
                  DefaultTemperature=0
                  InitialCrackSize=0.4
                  KRoughness=1
                  KTreatment=1
                  KUser=1
                  Material=Test_mat
                  ScaleFactor=1
                  ShapeFactor=<Not set>
                  StressOffset=0
                  StressOffsetUnits=MPa
                  SurfaceRoughness=0
                  SurfaceRoughnessType=Polished
                  WeldDiameter=<Not set>
                  WeldDiameterMethod=Auto
                  WeldDiameterUnits=mm
                  WeldLookupFilename=<Not set>
                }
                OBJECT ** MAT_2 ** (DTMaterialMapEntry : Material map entry)
                {
                  AdhesiveThickness=0.1
                  BondDistanceUnits=mm
                  BondLineOffset=0
                  CutEdgeLocation=None
                  DangVanParameterFilename=<Not set>
                  DatabaseName=<Not set>
                  DefaultMaterial=False
                  DefaultTemperature=0
                  InitialCrackSize=0.4
                  KRoughness=1
                  KTreatment=1
                  KUser=1
                  Material=Test_mat
                  ScaleFactor=1
                  ShapeFactor=<Not set>
                  StressOffset=0
                  StressOffsetUnits=MPa
                  SurfaceRoughness=0
                  SurfaceRoughnessType=Polished
                  WeldDiameter=<Not set>
                  WeldDiameterMethod=Auto
                  WeldDiameterUnits=mm
                  WeldLookupFilename=<Not set>
                }
              }
            }
            OBJECT ** gage ** (DTEntitySubsetDynamic : Dynamic entity subset)
            {
              EntityType=Nodes
              ProcessInOrder=False
            }
          }
        }
      }
    }
  }
  ATTACHMENTS to Job
  {
    OBJECT ** VibrationLoad ** (DTLoadProviderVibration : Vibration load provider)
    {
      ActionOnLargePowerRatio=Warn
      ClippingFactor=3
      ComplexAlgorithm=Exact
      ComplexAlgorithmMaxIterations=100
      ComplexAlgorithmPrecision=1E-12
      CycleCountBins=128
      DividerAllStaticLoadCases=<Not set>
      ExposureDuration=1
      Filename=
      FrequencyExtrapolationMethod=UseLimits
      FrequencyInterval=<Not set>
      FrequencySelectionMethod=FRFFrequencies
      InterpolationMethod=LogLog
      LoadingConfigSource=Custom
      LoadingMethod=SineSweep
      MaxFrequency=<Not set>
      MinFrequency=<Not set>
      ModalLoading=False
      NoiseFloor=-120
      NumberOfSweeps=1
      PSDCycleCountMethod=Lalanne
      ResultsSetName=
      ScaleFactorAllStaticLoadCases=<Not set>
      SigmaClipping=None
      SineDwellDurationDays=0
      SineDwellDurationHours=0
      SineDwellDurationSeconds=600
      SineDwellDurationYears=0
      SineDwellFrequency=10
      SineOnRandomAmplitudes=<Not set>
      SineOnRandomCycleCountMethod=NarrowBand
      SineOnRandomFrequencies=<Not set>
      SweepRate=1
      SweepType=LinearHzPerSec
      ATTACHMENTS to VibrationLoad
      {
        OBJECT ** HistogramPipe1 ** (DTHistogramPipe : Histogram input from pipe)
        {
        }
      }
    }
    VibrationLoadCase 1 FELoadCase=1 FELoadCase2=1 Selected Load: Vibration Generator Channel - HistogramPipe1 (c1)
    StaticLoadCase 1 FELoadCase=1 ScaleFactor=1 Divider=1 
    OBJECT ** FEResultsImport ** (DTFEResultsImport : Imported FE results)
    {
      IntermediateFilename=
      NumTranslationProcesses=2
      OneLoadCasePerProcess=False
      SaveIntermediate=True
      TranslateInSeparateProcess=True
      TranslationSplitMethod=Auto
      CHILDREN of FEResultsImport
      {
        OBJECT ** FRF Input ** (DTFEImportResultsSet : FE import results set)
        {
          Description=
          FEFilenames=c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\MECH\file.rst,c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-1\MECH\file.rst
          FEResults=Standard
          IgnoreMidsideNodes=False
          IncludeDisplacements=None
          IncludeEquivalentPlasticStrain=False
          IncludeTemperatures=False
          SelectionGroupType=FEInput
          StateVariableMappingFile=
          UserLoadSetFilename=
          UserLoadSetIDs=
          UserLoadSetType=FromIDs
          VibrationOffset=False
        }
        OBJECT ** Offset Loadcase Input ** (DTFEImportResultsSet : FE import results set)
        {
          Description=<Not set>
          FEFilenames=c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\MECH\file.rst,c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-1\MECH\file.rst
          FEResults=Standard
          IgnoreMidsideNodes=False
          IncludeDisplacements=None
          IncludeEquivalentPlasticStrain=False
          IncludeTemperatures=False
          SelectionGroupType=FEInput
          StateVariableMappingFile=
          UserLoadSetFilename=
          UserLoadSetIDs=
          UserLoadSetType=FromIDs
          VibrationOffset=True
        }
        OBJECT ** AnalysisGroup ** (DTFEImportAnalysisGroup : FE import analysis group)
        {
          AccelerationUnits=mm/s^2
          AdhesiveElementType=Beam
          AllowableFeatureAngle=20
          AverageResultsAtNodes=False
          CriticalDistance=0
          CriticalDistanceMethod=Point
          CriticalDistanceType=AveragedNodeOnElement
          Description=<Not set>
          DistanceUnits=mm
          EntityDataType=Vibration
          ExcludeRigidAttached=False
          ExtrapolationPoints=Two
          ForceUnits=N
          GroupNames=*
          IdentifyFreeEdges=False
          IgnoreZeroData=True
          IncludeSpotWeldCoordinates=False
          IncludeSpotWeldNuggets=True
          LargeDisplacements=False
          LowerFilletOverlapThreshold=30
          MaterialAssignmentGroup=Material
          MaterialOrientationTensor=None
          MaxWeldDepth=0
          MeshQuality=Fine
          MinimumRadiusOfCurvature=0.5
          MomentUnits=N.mm
          NumNotchWeldLines=1
          NumWeldLayers=5
          NumberOfPoints=5
          OffsetMethod=Default
          OffsetType=Ratio
          OffsetValues=0,0,0
          OrientationTensorFile=
          ResolveToLocal=True
          SeamWeldType=Fillet
          SelectionGroupType=FEInput
          SetEntityType=Element
          ShellLayer=TopAndBottom
          SolidLayer=All
          SolidWeldAuto=False
          SolutionLocation=AveragedNodeOnElement
          StateVariableKey=Macro
          StrainGaugeFilename=
          StrainGaugeSource=MetaData
          StrainUnits=strain
          StressGradients=False
          StressUnits=MPa
          SurfaceNodesOnly=True
          SymmetryAxis=Y
          SymmetryDefinitionFilename=
          SymmetryType=None
          TemperatureUnits=deg C
          UnitsDefinition=MPA,MM,N,TNMM,DEGC
          UpperFilletOverlapThreshold=60
          UseShear=False
          UserGroupsToExclude=
          UserSetFilename=
          UserSetIDs=
          UserSetType=FromIDs
          VelocityUnits=mm/s
          VirtualSensorFilename=
          VirtualSensorNodalSum=False
          VirtualSensorSource=MetaData
          WeldDefinitionFilename=
          WeldEndElements=Include
          WeldHotSpotElementType=Solid
          WeldOutputFilename=
          WeldResultLocation=NodeOnElement
        }
      }
    }
    OBJECT ** ResultsHandler ** (DTResultsHandlerFER : FER results handler)
    {
      ColumnsToIgnore=
      ColumnsToSave=ALL
      Filename=
      Overwrite=False
      SaveFile=False
      ATTACHMENTS to ResultsHandler
      {
        OBJECT ** Compressed results (for display) ** (DTPostProcessorPipe : Pipe post processor)
        {
          CategoryKeepCount=1
          CategoryKeyword=
          ChannelPerEvent=False
          Compress=True
          EnableProgressiveUpdate=False
          EquivUnits=Repeats
          IncludeSolids=True
          LayerFullCompression=True
          MinersSum=1
          NumEquivUnits=1
          OutputResultSource=False
          RunColumnOutput=Common
          RunCombination=Worst
          SavePropsToMetadata=False
          ShellLayer=All
          SortKeywords=-Damage
        }
      }
    }
  }
}
   
   
   
Unable to locate 'post run' property set in run 0 audit
Product         GlyphWorks V25.0.0 Release Build 431
Platform        Windows64
abcdlib         V25.0 A01 Jan 14 2025 12:42:50
ailib           V25.0 A01 Jan 14 2025 12:43:34
Ans.DesignLifeAddin V25.1 A00 Tuesday, January 14, 2025 1:48:14 PM
anslib          V25.0 A01 Jan 14 2025 12:43:19
asamlib         V25.0 A01 Jan 14 2025 13:07:33
atlib           V25.0 A01 Jan 14 2025 12:51:03
CBLib           V25.0 A01 Jan 14 2025 12:43:46
cgdlib          V25.0 A01 Jan 14 2025 12:48:23
cgflib          V25.0 A01 Jan 14 2025 12:41:16
cgolib          V25.0 A01 Jan 14 2025 12:48:07
cgrlib          V25.0 A01 Jan 14 2025 12:47:43
cpputil         V25.0 A01 Jan 14 2025 12:34:31
dglib           V25.0 A01 Jan 14 2025 12:50:00
dmilib          V25.0 A01 Jan 14 2025 12:35:37
dtlib           V25.0 A01 Jan 14 2025 12:47:07
extlib          V25.0 A01 Jan 14 2025 12:32:12
fatlib          V25.0 A01 Jan 14 2025 12:39:41
FDLib           V25.0 A01 Jan 14 2025 12:44:23
fedlib          V25.0 A01 Jan 14 2025 12:53:52
feilib          V25.0 A01 Jan 14 2025 12:43:08
feimportlib (ANSYS) V25.0 A01 Jan 14 2025 12:46:38
ferlib          V25.0 A01 Jan 14 2025 12:37:58
fiolib          V25.0 A01 Jan 14 2025 12:42:00
FSLib           V25.0 A01 Jan 14 2025 12:37:05
FVLib           V25.0 A01 Jan 14 2025 12:56:58
GlyphEngine01   V25.0 A01 Jan 14 2025 12:59:10
GlyphEngine02   V25.0 A01 Jan 14 2025 12:59:49
GlyphEngine03   V25.0 A01 Jan 14 2025 13:00:38
GlyphEngine04   V25.0 A01 Jan 14 2025 13:01:39
GlyphEngine06   V25.0 A01 Jan 14 2025 13:02:36
GlyphEngine07   V25.0 A01 Jan 14 2025 13:03:02
GlyphEngine08   V25.0 A01 Jan 14 2025 13:03:23
GlyphEngine09   V25.0 A01 Jan 14 2025 13:03:48
GlyphEngine10   V25.0 A01 Jan 14 2025 13:04:14
GlyphEngine13   V25.0 A01 Jan 14 2025 13:04:39
GlyphEngine14   V25.0 A01 Jan 14 2025 13:05:28
GlyphEngine15   V25.0 A01 Jan 14 2025 13:05:56
GlyphEngine16   V25.0 A01 Jan 14 2025 13:06:24
grlib           V25.0 A01 Jan 14 2025 12:51:53
gutlib          V25.0 A01 Jan 14 2025 12:55:50
iceintlib       V25.0 A01 Jan 14 2025 12:50:33
IXDLib          V25.0 A01 Jan 14 2025 12:35:52
jprolib         V25.0 A01 Jan 14 2025 12:42:35
lican           V25.0 A01 Jan 14 2025 12:30:34
licnc           V25.0 A01 Jan 14 2025 12:30:19
licsh           V25.0 A01 Jan 14 2025 12:30:10
maplib          V25.0 A01 Jan 14 2025 12:35:25
matdblib        V25.0 A01 Jan 14 2025 12:38:15
materials       V25.0 A01 Jan 14 2025 12:49:26
mcxlib          V25.0 A01 Jan 14 2025 12:32:51
mthlib          V25.0 A01 Jan 14 2025 12:35:14
mtlib           V25.0 A01 Jan 14 2025 12:33:48
ncmpilib        V25.0 A01 Jan 14 2025 12:32:18
ncodedesktop    V25.0 A01 Jan 14 2025 13:27:32
ncxml           V25.0 A01 Jan 14 2025 12:30:42
nmxfiolib       V25.0 A01 Jan 14 2025 12:37:45
nulib           V25.0 A01 Jan 14 2025 12:34:46
NXLib           V25.0 A01 Jan 14 2025 12:33:01
PipeData00      V25.0 A01 Jan 14 2025 12:55:01
ProgramEngine00 V25.0 A01 Jan 14 2025 13:06:46
pylib           V25.0 A01 Jan 14 2025 12:33:57
QCLib           V25.0 A01 Jan 14 2025 12:55:21
qtutil          V25.0 A01 Jan 14 2025 12:48:50
QXLib           V25.0 A01 Jan 14 2025 12:45:08
S3Lib           V25.0 A01 Jan 14 2025 12:33:22
sielib          V25.0 A01 Jan 14 2025 12:37:35
siglib          V25.0 A01 Jan 14 2025 12:40:54
utlib (ANSYS)   V25.0 A01 Jan 14 2025 12:28:47
xllib           V25.0 A01 Jan 14 2025 12:31:01
Pre run audit data
   
Start time - 15-Aug-2025 15:16:15
Single run
Flow file - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-2\DL\dl.fdb
Glyph count - 17
   
   
Glyph 1 - "VibrationGenerator1"
Version - 5
   
Output connections - 1
Output connection 1:1 - Plug1.Vibration Profile to SweptSine_Analysis.Histogram.HistogramPipe1
Output connection 1:2 - Plug1.Vibration Profile to Swept Sine Display.HistSocket.s1b
   
Properties - 19 entries (pre-run state)
AdditionalNumberOfSweeps = 0
EndFrequency = 101
FrequencyStep = 1
InterpolationMethod = Log
Name = sine_sweep
NoiseFloor = -120
NumberOfBins = 1024
PSDUnits = Acceleration
SineAmplitudes = Undefined
SineFrequencies = Undefined
StartFrequency = 1
SweepRate = 1
SweepType = HZ/Sec (Linear)
TestDuration = 100
TestName = Undefined
TestType = Acceleration (g)
Type = SineSweep2
VibrationTable = PropertiesTab
XMLTables = <VibrationTables Version="1.0"><Tables><SineSweep/><SineDwell/><RandomPSD><RandomPSDItem Amplitude="1" Frequency="1"/><RandomPSDItem Amplitude="1" Frequency="1000"/></RandomPSD><SineOnRandom/><SineSweep2><SineSweep2Item Amplitude="0.1" Frequency="1"/><SineSweep2Item Amplitude="1" Frequency="10"/><SineSweep2Item Amplitude="1" Frequency="100"/></SineSweep2></Tables></VibrationTables>

   
   
Glyph 2 - "Bill_of_Materials_Input"
Version - 7
   
Input files - 1
Input file 1 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-2\DL\dlbom.csv;amc;c1
   
Output connections - 1
Output connection 1:1 - Plug1.P1a to SweptSine_Analysis.MaterialMapLoader.Use materials from Workbench
   
Properties - 7 entries (pre-run state)
CombineAllTests = False
DiscardProcessedTests = False
LoopAllTests = True
MatchingMethod = ChannelNumber
SVDecimalSeparator = 
SVSeparator = 
SaveTestList = False
   
   
Glyph 3 - "Simulation_Input"
Version - 8
   
Input files - 2
Input file 1 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\MECH\file.rst;afe;c1
Input file 2 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-1\MECH\file.rst;afe;c1
   
Output connections - 1
Output connection 1:1 - Plug1.FE Model Data to SweptSine_Analysis.FEMetaData.FRF Input
Output connection 1:2 - Plug1.FE Model Data to SweptSine_Analysis.FEMetaData.Offset Loadcase Input
   
Properties - 9 entries (pre-run state)
CombineTests = True
DiscardProcessedTests = False
ImportUserGroups = False
LoadCaseNumbering = EachFile
LoadCases = Undefined
LoopAllTests = True
SaveTestList = False
StoreDisplayedGroups = False
UserGroupsFilename = Undefined
   
   
Glyph 4 - "SweptSine_Analysis"
Version - 8
   
Input connections - 4
Input connection 1 - FEMetaData.FRF Input from Simulation_Input.Plug1.FE Model Data
Input connection 2 - FEMetaData.Offset Loadcase Input from Simulation_Input.Plug1.FE Model Data
Input connection 3 - MaterialMapLoader.Use materials from Workbench from Bill_of_Materials_Input.Plug1.P1a
Input connection 4 - Histogram.HistogramPipe1 from VibrationGenerator1.Plug1.Vibration Profile
   
Output connections - 4
Output connection 1:1 - Results.Compressed results (for display) to HotSpotDetection1.CAE Fatigue Results.CAE Fatigue Results
Output connection 1:2 - Results.Compressed results (for display) to FER_File_Output.S1.S1a
Output connection 1:3 - Results.Compressed results (for display) to Fatigue_Results_Display.FE Results.FE Results
Output connection 1:4 - Results.Compressed results (for display) to MultiColumnFilter1.Socket1.Multi-Column Input
Output connection 1:5 - Results.Compressed results (for display) to DataValuesDisplay.S1.S1c
Output connection 1:6 - Results.Compressed results (for display) to Design Explorer Output1.Linked to SGInput1.Input 1
Output connection 2:1 - MultiColumn.PSD of Stress to Stress_Amplitude_Spectrum.MCSocket.Multi-Column Input 1
Output connection 3:1 - Histogram.Cycles Histogram to Cycles_Histogram.S1.Histogram Input 1
Output connection 4:1 - Histogram.Damage Histogram to Damage_Histogram.S1.Histogram Input 1
   
Properties - 23 entries (pre-run state)
AnalysisGroup_GroupNames = *
AnalysisGroup_MaterialAssignmentGroup = Material
AnalysisGroup_SelectionGroupType = FEInput
AnalysisGroup_ShellLayer = TopAndBottom
AnalysisGroup_SolutionLocation = AveragedNodeOnElement
AnalysisGroup_UnitsDefinition = MPA,MM,N,TNMM,DEGC
Job_NumAnalysisThreads = ?
LogMessageLimit = 100
LoggingLevel = Info
ResultsUpdateInterval = 10
SNEngine_CertaintyOfSurvival = 50
SNEngine_CombinationMethod = AbsMaxPrincipal
SNEngine_MeanStressCorrection = Interpolate
SNEngine_SNMethod = MultiRRatioCurve
Use materials from Workbench_Active = True
VibrationLoad_FrequencySelectionMethod = FRFFrequencies
VibrationLoad_InterpolationMethod = LogLog
VibrationLoad_LoadingMethod = SineSweep
VibrationLoad_SineDwellDurationSeconds = 600
VibrationLoad_SineDwellFrequency = 10
VibrationLoad_SweepRate = 1
VibrationLoad_SweepType = LinearHzPerSec
matml_DatabaseName = C:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\ENGD\material.engd
   
   
Glyph 5 - "HotSpotDetection1"
Version - 3
   
Input connections - 1
Input connection 1 - CAE Fatigue Results.CAE Fatigue Results from SweptSine_Analysis.Results.Compressed results (for display)
   
Output connections - 1
Output connection 1:1 - Hot Spot List.Hot Spot List to HotSpot_List_Output.Socket1.S1a
Output connection 1:2 - Hot Spot List.Hot Spot List to Fatigue_Results_Display.Feature List.Hot Spot List
   
Properties - 9 entries (pre-run state)
CategoryColumnKeyword = Undefined
ColumnsToOutput = Undefined
EntityType = Auto
HotSpotDataKeyword = Damage
HotSpotPeakDirection = Max
IncludeAdjacentLocations = False
MaxNumCategories = 100
MaxNumHotSpots = 10
ProcessByCategory = False
   
   
Glyph 6 - "FER_File_Output"
Version - 8
   
Input connections - 1
Input connection 1 - S1.S1a from SweptSine_Analysis.Results.Compressed results (for display)
   
Properties - 21 entries (pre-run state)
CategoryKeepCount = 1
CategoryKeyword = Undefined
CompressResults = True
EquivUnits = Repeats
EventNaming = Name
ExportCSVDecimalSeparator = 
ExportCSVSeparator = 
GroupType = Property
IncludeSolids = True
MaxGroups = 1000
MinersSum = 1
MultipleEventsSingleODB = False
NodeOnElementCompression = Element
NumEquivUnits = 1
ODBInputFilename = Undefined
OutputFilename = #Test.InputTestInfo.TestName#
OutputFormat = nCode_FER
Overwrite = Yes
Record4ConfigFile = 
ShellLayer = Worst
SortKeywords = -damage
   
   
Glyph 7 - "HotSpot_List_Output"
Version - 4
   
Input connections - 1
Input connection 1 - Socket1.S1a from HotSpotDetection1.Hot Spot List.Hot Spot List
   
Properties - 13 entries (pre-run state)
ASAMDataModel = Undefined
AddToFileList = False
ClearInputGlyphFiles = True
EnumOutput = String
ExportSVDecimalSeparator = 
ExportSVSeparator = 
FileFormat = S3MultiColumn
LoadOutputFilesIntoInputGlyph = 
MetaDataOutput = SaveWithTest
NameText = HotSpot_List
NamingMethod = NewName
Overwrite = Yes
WriteMetadataToSV = False
   
   
Glyph 8 - "Fatigue_Results_Display"
Version - 2
   
Input connections - 2
Input connection 1 - FE Results.FE Results from SweptSine_Analysis.Results.Compressed results (for display)
Input connection 2 - Feature List.Hot Spot List from HotSpotDetection1.Hot Spot List.Hot Spot List
   
Properties - 1 entries (pre-run state)
ModelFilename = 
   
   
Glyph 9 - "Swept Sine Display"
Version - 1
   
Input connections - 1
Input connection 1 - HistSocket.s1b from VibrationGenerator1.Plug1.Vibration Profile
   
Properties - 30 entries (pre-run state)
CursorOutput = None
CursorReceive = None
CursorSend = None
HarmonicXCursors = None
LegendHeightPercent = 25
NameTextInput1 = _in1
NameTextInput2 = _in2
NameTextInput3 = _in3
NameTextInput4 = _in4
NameTextInput5 = _in5
NameTextInput6 = _in6
NameTextInput7 = _in7
NameTextInput8 = _in8
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
NamingMethodInput3 = Suffix
NamingMethodInput4 = Suffix
NamingMethodInput5 = Suffix
NamingMethodInput6 = Suffix
NamingMethodInput7 = Suffix
NamingMethodInput8 = Suffix
NumHistogramInputPads = 2
NumMultiColumnInputPads = 2
NumTsInputPads = 2
NumberPeakCursors = 3
PeakXcursors = None
ShowLegend = False
StoreCursors = False
XCursors = 
YCursors = 
   
   
Glyph 10 - "Cycles_Histogram"
Version - 1
   
Input connections - 1
Input connection 1 - S1.Histogram Input 1 from SweptSine_Analysis.Histogram.Cycles Histogram
   
Properties - 4 entries (pre-run state)
NameTextInput1 = _in1
NameTextInput2 = _in2
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
   
   
Glyph 11 - "Stress_Amplitude_Spectrum"
Version - 1
   
Input connections - 1
Input connection 1 - MCSocket.Multi-Column Input 1 from SweptSine_Analysis.MultiColumn.PSD of Stress
   
Properties - 30 entries (pre-run state)
CursorOutput = None
CursorReceive = CursorA
CursorSend = CursorA
HarmonicXCursors = None
LegendHeightPercent = 25
NameTextInput1 = _in1
NameTextInput2 = _in2
NameTextInput3 = _in3
NameTextInput4 = _in4
NameTextInput5 = _in5
NameTextInput6 = _in6
NameTextInput7 = _in7
NameTextInput8 = _in8
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
NamingMethodInput3 = Suffix
NamingMethodInput4 = Suffix
NamingMethodInput5 = Suffix
NamingMethodInput6 = Suffix
NamingMethodInput7 = Suffix
NamingMethodInput8 = Suffix
NumHistogramInputPads = 2
NumMultiColumnInputPads = 2
NumTsInputPads = 2
NumberPeakCursors = 3
PeakXcursors = None
ShowLegend = False
StoreCursors = True
XCursors = Undefined
YCursors = Undefined
   
   
Glyph 12 - "Damage_Histogram"
Version - 1
   
Input connections - 1
Input connection 1 - S1.Histogram Input 1 from SweptSine_Analysis.Histogram.Damage Histogram
   
Properties - 4 entries (pre-run state)
NameTextInput1 = _in1
NameTextInput2 = _in2
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
   
   
Glyph 13 - "MultiColumnFilter1"
Version - 1
   
Input connections - 1
Input connection 1 - Socket1.Multi-Column Input from SweptSine_Analysis.Results.Compressed results (for display)
   
Output connections - 1
Output connection 1:1 - Plug1.Multi-Column Output to CSV_File_Output.S1.S1a
   
Properties - 7 entries (pre-run state)
Channels = Undefined
ColumnsToExclude = Undefined
ColumnsToInclude = NodeID,Damage,Life
FilterCaseSensitive = False
FilterColumn = Undefined
FilterComparison = =
FilterValue = Undefined
   
   
Glyph 14 - "CSV_File_Output"
Version - 8
   
Input connections - 1
Input connection 1 - S1.S1a from MultiColumnFilter1.Plug1.Multi-Column Output
   
Properties - 21 entries (pre-run state)
CategoryKeepCount = 1
CategoryKeyword = Undefined
CompressResults = True
EquivUnits = Repeats
EventNaming = Name
ExportCSVDecimalSeparator = 
ExportCSVSeparator = 
GroupType = Property
IncludeSolids = True
MaxGroups = 1000
MinersSum = 1
MultipleEventsSingleODB = False
NodeOnElementCompression = Element
NumEquivUnits = 1
ODBInputFilename = Undefined
OutputFilename = dl_results
OutputFormat = CSV
Overwrite = Yes
Record4ConfigFile = 
ShellLayer = Worst
SortKeywords = -damage
   
   
Glyph 15 - "DX_parameters"
Version - 1
   
Output connections - 1
Output connection 1:1 - Output.Metadata Output to Design Explorer Output1.Linked to SGInput1.Metadata Input
   
Properties - 4 entries (pre-run state)
HideSetupTabs = True
Parameter_per_group = False
Parameter_type = life
Properties = <Properties><Property help="If True, a parameter for each material group is exported. If False a single parameter for the entire model is exported." name="Parameter_per_group" type="boolean" mandatory="true" description="Export a parameter for each material group, or a single parameter for the model"/><Property help="The worst result of this type will be passed back to DesignExplorer. Fatigue analyses for damage can export either life or damage. Backcalculation analyses can export scalefactor, and DangVan can export safetyfactor. On a dutycycle run, the total schedule results is used." name="Parameter_type" type="enum" enumopts="damage,life,safetyfactor,scalefactor" mandatory="true" description="Type of fatigue result to pass to DesignExplorer"/></Properties>
   
   
Glyph 16 - "Design Explorer Output1"
Version - 1
   
Input connections - 2
Input connection 1 - Linked to SGInput1.Input 1 from SweptSine_Analysis.Results.Compressed results (for display)
Input connection 2 - Linked to SGInput1.Metadata Input from DX_parameters.Output.Metadata Output
   
Properties - 5 entries (pre-run state)
BitmapFileName = SuperGlyph
IconFileName = SuperGlyph
Locked = False
Verbose = True
   
   
Glyph 17 - "DataValuesDisplay"
Version - 13
   
Input connections - 1
Input connection 1 - S1.S1c from SweptSine_Analysis.Results.Compressed results (for display)
   
Properties - 33 entries (pre-run state)
2DHistogramVerticalFormat = True
ChannelsToDisplay = Undefined
ColumnLabel = AxisTitle
Columns = 
ColumnsToColour = 
DisplayMode = Mag/Phase
EqualsColour = LightGreen
EqualsTolerance = 1E-4
EqualsValue = ?
ExportCSVDecimalSeparator = 
ExportCSVSeparator = 
ExportNameText = Undefined
ExportNamingMethod = Suffix
ExportType = None
HistogramBinLabels = BinCentre
IntegerFormat = Decimal
IntervalUnits = Point
LowerGate = ?
LowerGateColour = Blue
MaximumValueColour = Undefined
MinimumValueColour = Undefined
MissingValuesSpace = True
NumberSigFig = 4
Overwrite = Ask
PointIncrementValue = 10
ReverseYAxis = False
ShowColumnKeywords = False
ShowColumnTypes = False
TransposeXY = Normal
UTCFormat = Local
UpperGate = ?
UpperGateColour = Red
XAxisUnitsIncrementValue = 1
   
   
   
   
   
In run audit data
   
   
Glyph 1 - "VibrationGenerator1"
   
Glyph 2 - "Bill_of_Materials_Input"
   
Glyph 3 - "Simulation_Input"
   
Glyph 4 - "SweptSine_Analysis"
   
Glyph 5 - "HotSpotDetection1"
   
Glyph 6 - "FER_File_Output"
   
Glyph 7 - "HotSpot_List_Output"
   
Glyph 8 - "Fatigue_Results_Display"
   
Glyph 9 - "Swept Sine Display"
   
Glyph 10 - "Cycles_Histogram"
   
Glyph 11 - "Stress_Amplitude_Spectrum"
   
Glyph 12 - "Damage_Histogram"
   
Glyph 13 - "MultiColumnFilter1"
   
Glyph 14 - "CSV_File_Output"
   
Glyph 15 - "DX_parameters"
   
Glyph 16 - "Design Explorer Output1"
2 info messages
Info 1 - . > Design Explorer Output1 (n=1)
Info 2 - . < Design Explorer Output1 (n=1) 0.3749secs
   
Glyph 17 - "DataValuesDisplay"
   
   
   
   
"Job" - 7 entries
"AuditFilename" = Undefined
"Description" = 
"IgnoreUnusedArguments" = False
"MemoryLogging" = False
"NumAnalysisThreads" = ?
"OverwriteAuditFile" = Append
"ValidateAutoConfigureLoading" = Warn
   
"SweptSine_Analysis" - 1 entries
"CAEConfiguration" = 
OBJECT ** Job ** (DTJob : Job)
{
  AuditFilename=<Not set>
  Description=
  IgnoreUnusedArguments=False
  MemoryLogging=False
  NumAnalysisThreads=<Not set>
  OverwriteAuditFile=Append
  ValidateAutoConfigureLoading=Warn
  CHILDREN of Job
  {
    OBJECT ** Run1 ** (DTRun : Run)
    {
      Gate=20
      GateUnits=Percent
      NumAnalysisThreads=<Not set>
      TimeHistoryCompression=None
      ATTACHMENTS to Run1
      {
        OBJECT ** AnaDef ** (DTAnalysisDefinition : Analysis definition)
        {
          AnalysisGroups=*
          AutoEliminationMode=False
          CompressionOverride=SameAsRun
          EntitySubsetCombination=<Not set>
          Gate=0
          GateUnits=Percent
          ATTACHMENTS to AnaDef
          {
            OBJECT ** SNEngine ** (DTAnalysisEngineSN : Standard SN analysis engine)
            {
              AngleInterval=10
              BackCalcAccuracy=1
              BackCalcMaxScale=5
              BackCalcMinScale=0.2
              BackCalcMode=None
              BiaxialityGate=20
              BiaxialityThresholdLower=-0.6
              BiaxialityThresholdUpper=0.6
              CertaintyOfSurvival=50
              CheckStaticFailure=False
              CombinationMethod=AbsMaxPrincipal
              CompressByMaxStress=False
              CustomSNMethod=CustomSNTest
              DamageFloor=1E-15
              EventProcessing=Independent
              FatigueReserveFactor=1
              InterpolationLimit=UseMaxCurve
              MaxDamage=1E30
              MeanStressCorrection=Interpolate
              MeanStressCorrectionStrengthParameter=YieldStrength
              MeanStressExponent=1
              MultiAxialAssessment=None
              NonPropFactorThreshold=0.25
              OutputDistributedSource=False
              OutputEventResults=False
              OutputMaterialNames=False
              OutputMaxMin=False
              OutputStats=False
              OutputStressGradientFactors=False
              OutputVibrationStats=False
              SNMethod=MultiRRatioCurve
              ScaleFactor=1
              ScaleNormalStress=False
              SmallCycleCorrection=None
              StaticFailureDamage=2
              StressGradientMethod=VonMises
              StressGradients=Auto
              StressGradientsUser=<Not set>
              TargetDamage=1E-6
              TemperatureInterpolationLimit=UseMaxCurve
              TemperatureSelection=CycleMax
              ZeroCompressiveDamage=Off
              ZeroDamageStressPercent=10
            }
            OBJECT ** MaterialMap ** (DTMaterialMap : Material map)
            {
              CSVFilename=
              DataSetType=nCodeSNRRatioCurveContainer
              DatabaseName=matml
              HideInternalMaterials=True
              MaterialSource=Database
              Permissions=Editable
              SaveMapping=True
              ValidateBeforeRun=False
              WeldLookupFilename=
              CHILDREN of MaterialMap
              {
                OBJECT ** Use materials from Workbench ** (DTMaterialMapLoaderPipe : Material map loader from pipe)
                {
                  Active=True
                  AdditionalDataKeys=Part,Material
                  ClearMap=True
                  MapEntryProperties=
                  MaterialGroupNameKeys=MaterialGroup
                  MaterialNameKey=Material
                }
                OBJECT ** MAT_1 ** (DTMaterialMapEntry : Material map entry)
                {
                  AdhesiveThickness=0.1
                  BondDistanceUnits=mm
                  BondLineOffset=0
                  CutEdgeLocation=None
                  DangVanParameterFilename=<Not set>
                  DatabaseName=<Not set>
                  DefaultMaterial=False
                  DefaultTemperature=0
                  InitialCrackSize=0.4
                  KRoughness=1
                  KTreatment=1
                  KUser=1
                  Material=Test_mat
                  ScaleFactor=1
                  ShapeFactor=<Not set>
                  StressOffset=0
                  StressOffsetUnits=MPa
                  SurfaceRoughness=0
                  SurfaceRoughnessType=Polished
                  WeldDiameter=<Not set>
                  WeldDiameterMethod=Auto
                  WeldDiameterUnits=mm
                  WeldLookupFilename=<Not set>
                }
                OBJECT ** MAT_2 ** (DTMaterialMapEntry : Material map entry)
                {
                  AdhesiveThickness=0.1
                  BondDistanceUnits=mm
                  BondLineOffset=0
                  CutEdgeLocation=None
                  DangVanParameterFilename=<Not set>
                  DatabaseName=<Not set>
                  DefaultMaterial=False
                  DefaultTemperature=0
                  InitialCrackSize=0.4
                  KRoughness=1
                  KTreatment=1
                  KUser=1
                  Material=Test_mat
                  ScaleFactor=1
                  ShapeFactor=<Not set>
                  StressOffset=0
                  StressOffsetUnits=MPa
                  SurfaceRoughness=0
                  SurfaceRoughnessType=Polished
                  WeldDiameter=<Not set>
                  WeldDiameterMethod=Auto
                  WeldDiameterUnits=mm
                  WeldLookupFilename=<Not set>
                }
              }
            }
            OBJECT ** PostProcessorElimination1 ** (DTPostProcessorElimination : Elimination post processor)
            {
              CategoryKeyword=<Not set>
              ColumnsToOutput=
              CountToKeep=1
              EntitySubsetName=gage
              HotSpotPeakDirection=Max
              IncludeAdjacentLocations=False
              KeepMode=Auto
              Limit=<Not set>
              LowerLimit=<Not set>
              MaxNumCategories=100
              MaxNumHotSpots=5
              Mode=HighestCount
              PercentToKeep=10
              ResultKeyword=Damage
              SecondaryFilter=None
              SecondaryLimit=<Not set>
              UpperLimit=<Not set>
            }
          }
        }
      }
    }
    OBJECT ** matml ** (DTMaterialDatabasenCode : nCode material database)
    {
      DatabaseName=C:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\ENGD\material.engd
      DatabaseType=MML
    }
    OBJECT ** Run2 ** (DTRun : Run)
    {
      Gate=0
      GateUnits=Percent
      NumAnalysisThreads=<Not set>
      TimeHistoryCompression=None
      ATTACHMENTS to Run2
      {
        OBJECT ** AnalysisDefinition1 ** (DTAnalysisDefinition : Analysis definition)
        {
          AnalysisGroups=*
          AutoEliminationMode=False
          CompressionOverride=SameAsRun
          EntitySubsetCombination=<Not set>
          Gate=0
          GateUnits=Percent
          ATTACHMENTS to AnalysisDefinition1
          {
            OBJECT ** AnalysisEngineSN1 ** (DTAnalysisEngineSN : Standard SN analysis engine)
            {
              AngleInterval=10
              BackCalcAccuracy=1
              BackCalcMaxScale=5
              BackCalcMinScale=0.2
              BackCalcMode=None
              BiaxialityGate=20
              BiaxialityThresholdLower=-0.6
              BiaxialityThresholdUpper=0.6
              CertaintyOfSurvival=50
              CheckStaticFailure=False
              CombinationMethod=AbsMaxPrincipal
              CompressByMaxStress=False
              CustomSNMethod=None
              DamageFloor=0
              EventProcessing=Independent
              FatigueReserveFactor=1
              InterpolationLimit=UseMaxCurve
              MaxDamage=0
              MeanStressCorrection=Interpolate
              MeanStressCorrectionStrengthParameter=YieldStrength
              MeanStressExponent=1
              MultiAxialAssessment=None
              NonPropFactorThreshold=0.25
              OutputDistributedSource=False
              OutputEventResults=False
              OutputMaterialNames=False
              OutputMaxMin=False
              OutputStats=False
              OutputStressGradientFactors=False
              OutputVibrationStats=False
              SNMethod=MultiRRatioCurve
              ScaleFactor=1
              ScaleNormalStress=False
              SmallCycleCorrection=None
              StaticFailureDamage=2
              StressGradientMethod=VonMises
              StressGradients=Auto
              StressGradientsUser=<Not set>
              TargetDamage=1E-6
              TemperatureInterpolationLimit=UseMaxCurve
              TemperatureSelection=CycleMax
              ZeroCompressiveDamage=Off
              ZeroDamageStressPercent=0
              ATTACHMENTS to AnalysisEngineSN1
              {
                OBJECT ** VibrationPSDOutput1 ** (DTVibrationPSDOutput : Vibration PSD output)
                {
                  ATTACHMENTS to VibrationPSDOutput1
                  {
                    OBJECT ** PSD of Stress ** (DTMultiColumnOutputPipe : Multi-column output to pipe)
                    {
                    }
                  }
                }
                OBJECT ** Cycles Histogram ** (DTHistogramOutputPipe : Histogram output to pipe)
                {
                  HistogramType=Rainflow
                }
                OBJECT ** Damage Histogram ** (DTHistogramOutputPipe : Histogram output to pipe)
                {
                  HistogramType=Damage
                }
              }
            }
            OBJECT ** MaterialMap ** (DTMaterialMap : Material map)
            {
              CSVFilename=
              DataSetType=nCodeSNRRatioCurveContainer
              DatabaseName=matml
              HideInternalMaterials=True
              MaterialSource=Database
              Permissions=Editable
              SaveMapping=True
              ValidateBeforeRun=False
              WeldLookupFilename=
              CHILDREN of MaterialMap
              {
                OBJECT ** Use materials from Workbench ** (DTMaterialMapLoaderPipe : Material map loader from pipe)
                {
                  Active=True
                  AdditionalDataKeys=Part,Material
                  ClearMap=True
                  MapEntryProperties=
                  MaterialGroupNameKeys=MaterialGroup
                  MaterialNameKey=Material
                }
                OBJECT ** MAT_1 ** (DTMaterialMapEntry : Material map entry)
                {
                  AdhesiveThickness=0.1
                  BondDistanceUnits=mm
                  BondLineOffset=0
                  CutEdgeLocation=None
                  DangVanParameterFilename=<Not set>
                  DatabaseName=<Not set>
                  DefaultMaterial=False
                  DefaultTemperature=0
                  InitialCrackSize=0.4
                  KRoughness=1
                  KTreatment=1
                  KUser=1
                  Material=Test_mat
                  ScaleFactor=1
                  ShapeFactor=<Not set>
                  StressOffset=0
                  StressOffsetUnits=MPa
                  SurfaceRoughness=0
                  SurfaceRoughnessType=Polished
                  WeldDiameter=<Not set>
                  WeldDiameterMethod=Auto
                  WeldDiameterUnits=mm
                  WeldLookupFilename=<Not set>
                }
                OBJECT ** MAT_2 ** (DTMaterialMapEntry : Material map entry)
                {
                  AdhesiveThickness=0.1
                  BondDistanceUnits=mm
                  BondLineOffset=0
                  CutEdgeLocation=None
                  DangVanParameterFilename=<Not set>
                  DatabaseName=<Not set>
                  DefaultMaterial=False
                  DefaultTemperature=0
                  InitialCrackSize=0.4
                  KRoughness=1
                  KTreatment=1
                  KUser=1
                  Material=Test_mat
                  ScaleFactor=1
                  ShapeFactor=<Not set>
                  StressOffset=0
                  StressOffsetUnits=MPa
                  SurfaceRoughness=0
                  SurfaceRoughnessType=Polished
                  WeldDiameter=<Not set>
                  WeldDiameterMethod=Auto
                  WeldDiameterUnits=mm
                  WeldLookupFilename=<Not set>
                }
              }
            }
            OBJECT ** gage ** (DTEntitySubsetDynamic : Dynamic entity subset)
            {
              EntityType=Nodes
              ProcessInOrder=False
            }
          }
        }
      }
    }
  }
  ATTACHMENTS to Job
  {
    OBJECT ** VibrationLoad ** (DTLoadProviderVibration : Vibration load provider)
    {
      ActionOnLargePowerRatio=Warn
      ClippingFactor=3
      ComplexAlgorithm=Exact
      ComplexAlgorithmMaxIterations=100
      ComplexAlgorithmPrecision=1E-12
      CycleCountBins=128
      DividerAllStaticLoadCases=<Not set>
      ExposureDuration=1
      Filename=
      FrequencyExtrapolationMethod=UseLimits
      FrequencyInterval=<Not set>
      FrequencySelectionMethod=FRFFrequencies
      InterpolationMethod=LogLog
      LoadingConfigSource=Custom
      LoadingMethod=SineSweep
      MaxFrequency=<Not set>
      MinFrequency=<Not set>
      ModalLoading=False
      NoiseFloor=-120
      NumberOfSweeps=1
      PSDCycleCountMethod=Lalanne
      ResultsSetName=
      ScaleFactorAllStaticLoadCases=<Not set>
      SigmaClipping=None
      SineDwellDurationDays=0
      SineDwellDurationHours=0
      SineDwellDurationSeconds=600
      SineDwellDurationYears=0
      SineDwellFrequency=10
      SineOnRandomAmplitudes=<Not set>
      SineOnRandomCycleCountMethod=NarrowBand
      SineOnRandomFrequencies=<Not set>
      SweepRate=1
      SweepType=LinearHzPerSec
      ATTACHMENTS to VibrationLoad
      {
        OBJECT ** HistogramPipe1 ** (DTHistogramPipe : Histogram input from pipe)
        {
        }
      }
    }
    VibrationLoadCase 1 FELoadCase=1 FELoadCase2=1 Selected Load: Vibration Generator Channel - HistogramPipe1 (c1)
    StaticLoadCase 1 FELoadCase=1 ScaleFactor=1 Divider=1 
    OBJECT ** FEResultsImport ** (DTFEResultsImport : Imported FE results)
    {
      IntermediateFilename=
      NumTranslationProcesses=2
      OneLoadCasePerProcess=False
      SaveIntermediate=True
      TranslateInSeparateProcess=True
      TranslationSplitMethod=Auto
      CHILDREN of FEResultsImport
      {
        OBJECT ** FRF Input ** (DTFEImportResultsSet : FE import results set)
        {
          Description=
          FEFilenames=c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\MECH\file.rst,c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-1\MECH\file.rst
          FEResults=Standard
          IgnoreMidsideNodes=False
          IncludeDisplacements=None
          IncludeEquivalentPlasticStrain=False
          IncludeTemperatures=False
          SelectionGroupType=FEInput
          StateVariableMappingFile=
          UserLoadSetFilename=
          UserLoadSetIDs=
          UserLoadSetType=FromIDs
          VibrationOffset=False
        }
        OBJECT ** Offset Loadcase Input ** (DTFEImportResultsSet : FE import results set)
        {
          Description=<Not set>
          FEFilenames=c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\MECH\file.rst,c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-1\MECH\file.rst
          FEResults=Standard
          IgnoreMidsideNodes=False
          IncludeDisplacements=None
          IncludeEquivalentPlasticStrain=False
          IncludeTemperatures=False
          SelectionGroupType=FEInput
          StateVariableMappingFile=
          UserLoadSetFilename=
          UserLoadSetIDs=
          UserLoadSetType=FromIDs
          VibrationOffset=True
        }
        OBJECT ** AnalysisGroup ** (DTFEImportAnalysisGroup : FE import analysis group)
        {
          AccelerationUnits=mm/s^2
          AdhesiveElementType=Beam
          AllowableFeatureAngle=20
          AverageResultsAtNodes=False
          CriticalDistance=0
          CriticalDistanceMethod=Point
          CriticalDistanceType=AveragedNodeOnElement
          Description=<Not set>
          DistanceUnits=mm
          EntityDataType=Vibration
          ExcludeRigidAttached=False
          ExtrapolationPoints=Two
          ForceUnits=N
          GroupNames=*
          IdentifyFreeEdges=False
          IgnoreZeroData=True
          IncludeSpotWeldCoordinates=False
          IncludeSpotWeldNuggets=True
          LargeDisplacements=False
          LowerFilletOverlapThreshold=30
          MaterialAssignmentGroup=Material
          MaterialOrientationTensor=None
          MaxWeldDepth=0
          MeshQuality=Fine
          MinimumRadiusOfCurvature=0.5
          MomentUnits=N.mm
          NumNotchWeldLines=1
          NumWeldLayers=5
          NumberOfPoints=5
          OffsetMethod=Default
          OffsetType=Ratio
          OffsetValues=0,0,0
          OrientationTensorFile=
          ResolveToLocal=True
          SeamWeldType=Fillet
          SelectionGroupType=FEInput
          SetEntityType=Element
          ShellLayer=TopAndBottom
          SolidLayer=All
          SolidWeldAuto=False
          SolutionLocation=AveragedNodeOnElement
          StateVariableKey=Macro
          StrainGaugeFilename=
          StrainGaugeSource=MetaData
          StrainUnits=strain
          StressGradients=False
          StressUnits=MPa
          SurfaceNodesOnly=True
          SymmetryAxis=Y
          SymmetryDefinitionFilename=
          SymmetryType=None
          TemperatureUnits=deg C
          UnitsDefinition=MPA,MM,N,TNMM,DEGC
          UpperFilletOverlapThreshold=60
          UseShear=False
          UserGroupsToExclude=
          UserSetFilename=
          UserSetIDs=
          UserSetType=FromIDs
          VelocityUnits=mm/s
          VirtualSensorFilename=
          VirtualSensorNodalSum=False
          VirtualSensorSource=MetaData
          WeldDefinitionFilename=
          WeldEndElements=Include
          WeldHotSpotElementType=Solid
          WeldOutputFilename=
          WeldResultLocation=NodeOnElement
        }
      }
    }
    OBJECT ** ResultsHandler ** (DTResultsHandlerFER : FER results handler)
    {
      ColumnsToIgnore=
      ColumnsToSave=ALL
      Filename=
      Overwrite=False
      SaveFile=False
      ATTACHMENTS to ResultsHandler
      {
        OBJECT ** Compressed results (for display) ** (DTPostProcessorPipe : Pipe post processor)
        {
          CategoryKeepCount=1
          CategoryKeyword=
          ChannelPerEvent=False
          Compress=True
          EnableProgressiveUpdate=False
          EquivUnits=Repeats
          IncludeSolids=True
          LayerFullCompression=True
          MinersSum=1
          NumEquivUnits=1
          OutputResultSource=False
          RunColumnOutput=Common
          RunCombination=Worst
          SavePropsToMetadata=False
          ShellLayer=All
          SortKeywords=-Damage
        }
      }
    }
  }
}
   
   
   
Unable to locate 'post run' property set in run 0 audit
Product         GlyphWorks V25.0.0 Release Build 431
Platform        Windows64
abcdlib         V25.0 A01 Jan 14 2025 12:42:50
ailib           V25.0 A01 Jan 14 2025 12:43:34
Ans.DesignLifeAddin V25.1 A00 Tuesday, January 14, 2025 1:48:14 PM
anslib          V25.0 A01 Jan 14 2025 12:43:19
asamlib         V25.0 A01 Jan 14 2025 13:07:33
atlib           V25.0 A01 Jan 14 2025 12:51:03
CBLib           V25.0 A01 Jan 14 2025 12:43:46
cgdlib          V25.0 A01 Jan 14 2025 12:48:23
cgflib          V25.0 A01 Jan 14 2025 12:41:16
cgolib          V25.0 A01 Jan 14 2025 12:48:07
cgrlib          V25.0 A01 Jan 14 2025 12:47:43
cpputil         V25.0 A01 Jan 14 2025 12:34:31
dglib           V25.0 A01 Jan 14 2025 12:50:00
dmilib          V25.0 A01 Jan 14 2025 12:35:37
dtlib           V25.0 A01 Jan 14 2025 12:47:07
extlib          V25.0 A01 Jan 14 2025 12:32:12
fatlib          V25.0 A01 Jan 14 2025 12:39:41
FDLib           V25.0 A01 Jan 14 2025 12:44:23
fedlib          V25.0 A01 Jan 14 2025 12:53:52
feilib          V25.0 A01 Jan 14 2025 12:43:08
feimportlib (ANSYS) V25.0 A01 Jan 14 2025 12:46:38
ferlib          V25.0 A01 Jan 14 2025 12:37:58
fiolib          V25.0 A01 Jan 14 2025 12:42:00
FSLib           V25.0 A01 Jan 14 2025 12:37:05
FVLib           V25.0 A01 Jan 14 2025 12:56:58
GlyphEngine01   V25.0 A01 Jan 14 2025 12:59:10
GlyphEngine02   V25.0 A01 Jan 14 2025 12:59:49
GlyphEngine03   V25.0 A01 Jan 14 2025 13:00:38
GlyphEngine04   V25.0 A01 Jan 14 2025 13:01:39
GlyphEngine06   V25.0 A01 Jan 14 2025 13:02:36
GlyphEngine07   V25.0 A01 Jan 14 2025 13:03:02
GlyphEngine08   V25.0 A01 Jan 14 2025 13:03:23
GlyphEngine09   V25.0 A01 Jan 14 2025 13:03:48
GlyphEngine10   V25.0 A01 Jan 14 2025 13:04:14
GlyphEngine13   V25.0 A01 Jan 14 2025 13:04:39
GlyphEngine14   V25.0 A01 Jan 14 2025 13:05:28
GlyphEngine15   V25.0 A01 Jan 14 2025 13:05:56
GlyphEngine16   V25.0 A01 Jan 14 2025 13:06:24
grlib           V25.0 A01 Jan 14 2025 12:51:53
gutlib          V25.0 A01 Jan 14 2025 12:55:50
iceintlib       V25.0 A01 Jan 14 2025 12:50:33
IXDLib          V25.0 A01 Jan 14 2025 12:35:52
jprolib         V25.0 A01 Jan 14 2025 12:42:35
lican           V25.0 A01 Jan 14 2025 12:30:34
licnc           V25.0 A01 Jan 14 2025 12:30:19
licsh           V25.0 A01 Jan 14 2025 12:30:10
maplib          V25.0 A01 Jan 14 2025 12:35:25
matdblib        V25.0 A01 Jan 14 2025 12:38:15
materials       V25.0 A01 Jan 14 2025 12:49:26
mcxlib          V25.0 A01 Jan 14 2025 12:32:51
mthlib          V25.0 A01 Jan 14 2025 12:35:14
mtlib           V25.0 A01 Jan 14 2025 12:33:48
ncmpilib        V25.0 A01 Jan 14 2025 12:32:18
ncodedesktop    V25.0 A01 Jan 14 2025 13:27:32
ncxml           V25.0 A01 Jan 14 2025 12:30:42
nmxfiolib       V25.0 A01 Jan 14 2025 12:37:45
nulib           V25.0 A01 Jan 14 2025 12:34:46
NXLib           V25.0 A01 Jan 14 2025 12:33:01
PipeData00      V25.0 A01 Jan 14 2025 12:55:01
ProgramEngine00 V25.0 A01 Jan 14 2025 13:06:46
pylib           V25.0 A01 Jan 14 2025 12:33:57
QCLib           V25.0 A01 Jan 14 2025 12:55:21
qtutil          V25.0 A01 Jan 14 2025 12:48:50
QXLib           V25.0 A01 Jan 14 2025 12:45:08
S3Lib           V25.0 A01 Jan 14 2025 12:33:22
sielib          V25.0 A01 Jan 14 2025 12:37:35
siglib          V25.0 A01 Jan 14 2025 12:40:54
utlib (ANSYS)   V25.0 A01 Jan 14 2025 12:28:47
xllib           V25.0 A01 Jan 14 2025 12:31:01
Pre run audit data
   
Start time - 15-Aug-2025 15:16:15
Single run
Flow file - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-2\DL\dl.fdb
Glyph count - 17
   
   
Glyph 1 - "VibrationGenerator1"
Version - 5
   
Output connections - 1
Output connection 1:1 - Plug1.Vibration Profile to SweptSine_Analysis.Histogram.HistogramPipe1
Output connection 1:2 - Plug1.Vibration Profile to Swept Sine Display.HistSocket.s1b
   
Properties - 19 entries (pre-run state)
AdditionalNumberOfSweeps = 0
EndFrequency = 101
FrequencyStep = 1
InterpolationMethod = Log
Name = sine_sweep
NoiseFloor = -120
NumberOfBins = 1024
PSDUnits = Acceleration
SineAmplitudes = Undefined
SineFrequencies = Undefined
StartFrequency = 1
SweepRate = 1
SweepType = HZ/Sec (Linear)
TestDuration = 100
TestName = Undefined
TestType = Acceleration (g)
Type = SineSweep2
VibrationTable = PropertiesTab
XMLTables = <VibrationTables Version="1.0"><Tables><SineSweep/><SineDwell/><RandomPSD><RandomPSDItem Amplitude="1" Frequency="1"/><RandomPSDItem Amplitude="1" Frequency="1000"/></RandomPSD><SineOnRandom/><SineSweep2><SineSweep2Item Amplitude="0.1" Frequency="1"/><SineSweep2Item Amplitude="1" Frequency="10"/><SineSweep2Item Amplitude="1" Frequency="100"/></SineSweep2></Tables></VibrationTables>

   
   
Glyph 2 - "Bill_of_Materials_Input"
Version - 7
   
Input files - 1
Input file 1 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-2\DL\dlbom.csv;amc;c1
   
Output connections - 1
Output connection 1:1 - Plug1.P1a to SweptSine_Analysis.MaterialMapLoader.Use materials from Workbench
   
Properties - 7 entries (pre-run state)
CombineAllTests = False
DiscardProcessedTests = False
LoopAllTests = True
MatchingMethod = ChannelNumber
SVDecimalSeparator = 
SVSeparator = 
SaveTestList = False
   
   
Glyph 3 - "Simulation_Input"
Version - 8
   
Input files - 2
Input file 1 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\MECH\file.rst;afe;c1
Input file 2 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-1\MECH\file.rst;afe;c1
   
Output connections - 1
Output connection 1:1 - Plug1.FE Model Data to SweptSine_Analysis.FEMetaData.FRF Input
Output connection 1:2 - Plug1.FE Model Data to SweptSine_Analysis.FEMetaData.Offset Loadcase Input
   
Properties - 9 entries (pre-run state)
CombineTests = True
DiscardProcessedTests = False
ImportUserGroups = False
LoadCaseNumbering = EachFile
LoadCases = Undefined
LoopAllTests = True
SaveTestList = False
StoreDisplayedGroups = False
UserGroupsFilename = Undefined
   
   
Glyph 4 - "SweptSine_Analysis"
Version - 8
   
Input connections - 4
Input connection 1 - FEMetaData.FRF Input from Simulation_Input.Plug1.FE Model Data
Input connection 2 - FEMetaData.Offset Loadcase Input from Simulation_Input.Plug1.FE Model Data
Input connection 3 - MaterialMapLoader.Use materials from Workbench from Bill_of_Materials_Input.Plug1.P1a
Input connection 4 - Histogram.HistogramPipe1 from VibrationGenerator1.Plug1.Vibration Profile
   
Output connections - 4
Output connection 1:1 - Results.Compressed results (for display) to HotSpotDetection1.CAE Fatigue Results.CAE Fatigue Results
Output connection 1:2 - Results.Compressed results (for display) to FER_File_Output.S1.S1a
Output connection 1:3 - Results.Compressed results (for display) to Fatigue_Results_Display.FE Results.FE Results
Output connection 1:4 - Results.Compressed results (for display) to MultiColumnFilter1.Socket1.Multi-Column Input
Output connection 1:5 - Results.Compressed results (for display) to DataValuesDisplay.S1.S1c
Output connection 1:6 - Results.Compressed results (for display) to Design Explorer Output1.Linked to SGInput1.Input 1
Output connection 2:1 - MultiColumn.PSD of Stress to Stress_Amplitude_Spectrum.MCSocket.Multi-Column Input 1
Output connection 3:1 - Histogram.Cycles Histogram to Cycles_Histogram.S1.Histogram Input 1
Output connection 4:1 - Histogram.Damage Histogram to Damage_Histogram.S1.Histogram Input 1
   
Properties - 23 entries (pre-run state)
AnalysisGroup_GroupNames = *
AnalysisGroup_MaterialAssignmentGroup = Material
AnalysisGroup_SelectionGroupType = FEInput
AnalysisGroup_ShellLayer = TopAndBottom
AnalysisGroup_SolutionLocation = AveragedNodeOnElement
AnalysisGroup_UnitsDefinition = MPA,MM,N,TNMM,DEGC
Job_NumAnalysisThreads = ?
LogMessageLimit = 100
LoggingLevel = Info
ResultsUpdateInterval = 10
SNEngine_CertaintyOfSurvival = 50
SNEngine_CombinationMethod = AbsMaxPrincipal
SNEngine_MeanStressCorrection = Interpolate
SNEngine_SNMethod = MultiRRatioCurve
Use materials from Workbench_Active = True
VibrationLoad_FrequencySelectionMethod = FRFFrequencies
VibrationLoad_InterpolationMethod = LogLog
VibrationLoad_LoadingMethod = SineSweep
VibrationLoad_SineDwellDurationSeconds = 600
VibrationLoad_SineDwellFrequency = 10
VibrationLoad_SweepRate = 1
VibrationLoad_SweepType = LinearHzPerSec
matml_DatabaseName = C:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\ENGD\material.engd
   
   
Glyph 5 - "HotSpotDetection1"
Version - 3
   
Input connections - 1
Input connection 1 - CAE Fatigue Results.CAE Fatigue Results from SweptSine_Analysis.Results.Compressed results (for display)
   
Output connections - 1
Output connection 1:1 - Hot Spot List.Hot Spot List to HotSpot_List_Output.Socket1.S1a
Output connection 1:2 - Hot Spot List.Hot Spot List to Fatigue_Results_Display.Feature List.Hot Spot List
   
Properties - 9 entries (pre-run state)
CategoryColumnKeyword = Undefined
ColumnsToOutput = Undefined
EntityType = Auto
HotSpotDataKeyword = Damage
HotSpotPeakDirection = Max
IncludeAdjacentLocations = False
MaxNumCategories = 100
MaxNumHotSpots = 10
ProcessByCategory = False
   
   
Glyph 6 - "FER_File_Output"
Version - 8
   
Input connections - 1
Input connection 1 - S1.S1a from SweptSine_Analysis.Results.Compressed results (for display)
   
Properties - 21 entries (pre-run state)
CategoryKeepCount = 1
CategoryKeyword = Undefined
CompressResults = True
EquivUnits = Repeats
EventNaming = Name
ExportCSVDecimalSeparator = 
ExportCSVSeparator = 
GroupType = Property
IncludeSolids = True
MaxGroups = 1000
MinersSum = 1
MultipleEventsSingleODB = False
NodeOnElementCompression = Element
NumEquivUnits = 1
ODBInputFilename = Undefined
OutputFilename = #Test.InputTestInfo.TestName#
OutputFormat = nCode_FER
Overwrite = Yes
Record4ConfigFile = 
ShellLayer = Worst
SortKeywords = -damage
   
   
Glyph 7 - "HotSpot_List_Output"
Version - 4
   
Input connections - 1
Input connection 1 - Socket1.S1a from HotSpotDetection1.Hot Spot List.Hot Spot List
   
Properties - 13 entries (pre-run state)
ASAMDataModel = Undefined
AddToFileList = False
ClearInputGlyphFiles = True
EnumOutput = String
ExportSVDecimalSeparator = 
ExportSVSeparator = 
FileFormat = S3MultiColumn
LoadOutputFilesIntoInputGlyph = 
MetaDataOutput = SaveWithTest
NameText = HotSpot_List
NamingMethod = NewName
Overwrite = Yes
WriteMetadataToSV = False
   
   
Glyph 8 - "Fatigue_Results_Display"
Version - 2
   
Input connections - 2
Input connection 1 - FE Results.FE Results from SweptSine_Analysis.Results.Compressed results (for display)
Input connection 2 - Feature List.Hot Spot List from HotSpotDetection1.Hot Spot List.Hot Spot List
   
Properties - 1 entries (pre-run state)
ModelFilename = 
   
   
Glyph 9 - "Swept Sine Display"
Version - 1
   
Input connections - 1
Input connection 1 - HistSocket.s1b from VibrationGenerator1.Plug1.Vibration Profile
   
Properties - 30 entries (pre-run state)
CursorOutput = None
CursorReceive = None
CursorSend = None
HarmonicXCursors = None
LegendHeightPercent = 25
NameTextInput1 = _in1
NameTextInput2 = _in2
NameTextInput3 = _in3
NameTextInput4 = _in4
NameTextInput5 = _in5
NameTextInput6 = _in6
NameTextInput7 = _in7
NameTextInput8 = _in8
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
NamingMethodInput3 = Suffix
NamingMethodInput4 = Suffix
NamingMethodInput5 = Suffix
NamingMethodInput6 = Suffix
NamingMethodInput7 = Suffix
NamingMethodInput8 = Suffix
NumHistogramInputPads = 2
NumMultiColumnInputPads = 2
NumTsInputPads = 2
NumberPeakCursors = 3
PeakXcursors = None
ShowLegend = False
StoreCursors = False
XCursors = 
YCursors = 
   
   
Glyph 10 - "Cycles_Histogram"
Version - 1
   
Input connections - 1
Input connection 1 - S1.Histogram Input 1 from SweptSine_Analysis.Histogram.Cycles Histogram
   
Properties - 4 entries (pre-run state)
NameTextInput1 = _in1
NameTextInput2 = _in2
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
   
   
Glyph 11 - "Stress_Amplitude_Spectrum"
Version - 1
   
Input connections - 1
Input connection 1 - MCSocket.Multi-Column Input 1 from SweptSine_Analysis.MultiColumn.PSD of Stress
   
Properties - 30 entries (pre-run state)
CursorOutput = None
CursorReceive = CursorA
CursorSend = CursorA
HarmonicXCursors = None
LegendHeightPercent = 25
NameTextInput1 = _in1
NameTextInput2 = _in2
NameTextInput3 = _in3
NameTextInput4 = _in4
NameTextInput5 = _in5
NameTextInput6 = _in6
NameTextInput7 = _in7
NameTextInput8 = _in8
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
NamingMethodInput3 = Suffix
NamingMethodInput4 = Suffix
NamingMethodInput5 = Suffix
NamingMethodInput6 = Suffix
NamingMethodInput7 = Suffix
NamingMethodInput8 = Suffix
NumHistogramInputPads = 2
NumMultiColumnInputPads = 2
NumTsInputPads = 2
NumberPeakCursors = 3
PeakXcursors = None
ShowLegend = False
StoreCursors = True
XCursors = Undefined
YCursors = Undefined
   
   
Glyph 12 - "Damage_Histogram"
Version - 1
   
Input connections - 1
Input connection 1 - S1.Histogram Input 1 from SweptSine_Analysis.Histogram.Damage Histogram
   
Properties - 4 entries (pre-run state)
NameTextInput1 = _in1
NameTextInput2 = _in2
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
   
   
Glyph 13 - "MultiColumnFilter1"
Version - 1
   
Input connections - 1
Input connection 1 - Socket1.Multi-Column Input from SweptSine_Analysis.Results.Compressed results (for display)
   
Output connections - 1
Output connection 1:1 - Plug1.Multi-Column Output to CSV_File_Output.S1.S1a
   
Properties - 7 entries (pre-run state)
Channels = Undefined
ColumnsToExclude = Undefined
ColumnsToInclude = NodeID,Damage,Life
FilterCaseSensitive = False
FilterColumn = Undefined
FilterComparison = =
FilterValue = Undefined
   
   
Glyph 14 - "CSV_File_Output"
Version - 8
   
Input connections - 1
Input connection 1 - S1.S1a from MultiColumnFilter1.Plug1.Multi-Column Output
   
Properties - 21 entries (pre-run state)
CategoryKeepCount = 1
CategoryKeyword = Undefined
CompressResults = True
EquivUnits = Repeats
EventNaming = Name
ExportCSVDecimalSeparator = 
ExportCSVSeparator = 
GroupType = Property
IncludeSolids = True
MaxGroups = 1000
MinersSum = 1
MultipleEventsSingleODB = False
NodeOnElementCompression = Element
NumEquivUnits = 1
ODBInputFilename = Undefined
OutputFilename = dl_results
OutputFormat = CSV
Overwrite = Yes
Record4ConfigFile = 
ShellLayer = Worst
SortKeywords = -damage
   
   
Glyph 15 - "DX_parameters"
Version - 1
   
Output connections - 1
Output connection 1:1 - Output.Metadata Output to Design Explorer Output1.Linked to SGInput1.Metadata Input
   
Properties - 4 entries (pre-run state)
HideSetupTabs = True
Parameter_per_group = False
Parameter_type = life
Properties = <Properties><Property help="If True, a parameter for each material group is exported. If False a single parameter for the entire model is exported." name="Parameter_per_group" type="boolean" mandatory="true" description="Export a parameter for each material group, or a single parameter for the model"/><Property help="The worst result of this type will be passed back to DesignExplorer. Fatigue analyses for damage can export either life or damage. Backcalculation analyses can export scalefactor, and DangVan can export safetyfactor. On a dutycycle run, the total schedule results is used." name="Parameter_type" type="enum" enumopts="damage,life,safetyfactor,scalefactor" mandatory="true" description="Type of fatigue result to pass to DesignExplorer"/></Properties>
   
   
Glyph 16 - "Design Explorer Output1"
Version - 1
   
Input connections - 2
Input connection 1 - Linked to SGInput1.Input 1 from SweptSine_Analysis.Results.Compressed results (for display)
Input connection 2 - Linked to SGInput1.Metadata Input from DX_parameters.Output.Metadata Output
   
Properties - 5 entries (pre-run state)
BitmapFileName = SuperGlyph
IconFileName = SuperGlyph
Locked = False
Verbose = True
   
   
Glyph 17 - "DataValuesDisplay"
Version - 13
   
Input connections - 1
Input connection 1 - S1.S1c from SweptSine_Analysis.Results.Compressed results (for display)
   
Properties - 33 entries (pre-run state)
2DHistogramVerticalFormat = True
ChannelsToDisplay = Undefined
ColumnLabel = AxisTitle
Columns = 
ColumnsToColour = 
DisplayMode = Mag/Phase
EqualsColour = LightGreen
EqualsTolerance = 1E-4
EqualsValue = ?
ExportCSVDecimalSeparator = 
ExportCSVSeparator = 
ExportNameText = Undefined
ExportNamingMethod = Suffix
ExportType = None
HistogramBinLabels = BinCentre
IntegerFormat = Decimal
IntervalUnits = Point
LowerGate = ?
LowerGateColour = Blue
MaximumValueColour = Undefined
MinimumValueColour = Undefined
MissingValuesSpace = True
NumberSigFig = 4
Overwrite = Ask
PointIncrementValue = 10
ReverseYAxis = False
ShowColumnKeywords = False
ShowColumnTypes = False
TransposeXY = Normal
UTCFormat = Local
UpperGate = ?
UpperGateColour = Red
XAxisUnitsIncrementValue = 1
   
   
   
   
   
In run audit data
   
   
Glyph 1 - "VibrationGenerator1"
   
Glyph 2 - "Bill_of_Materials_Input"
   
Glyph 3 - "Simulation_Input"
   
Glyph 4 - "SweptSine_Analysis"
   
Glyph 5 - "HotSpotDetection1"
   
Glyph 6 - "FER_File_Output"
   
Glyph 7 - "HotSpot_List_Output"
   
Glyph 8 - "Fatigue_Results_Display"
   
Glyph 9 - "Swept Sine Display"
   
Glyph 10 - "Cycles_Histogram"
   
Glyph 11 - "Stress_Amplitude_Spectrum"
   
Glyph 12 - "Damage_Histogram"
   
Glyph 13 - "MultiColumnFilter1"
   
Glyph 14 - "CSV_File_Output"
   
Glyph 15 - "DX_parameters"
   
Glyph 16 - "Design Explorer Output1"
2 info messages
Info 1 - . > Design Explorer Output1 (n=1)
Info 2 - . < Design Explorer Output1 (n=1) 0.3749secs
   
Glyph 17 - "DataValuesDisplay"
   
   
   
   
"Job" - 7 entries
"AuditFilename" = Undefined
"Description" = 
"IgnoreUnusedArguments" = False
"MemoryLogging" = False
"NumAnalysisThreads" = ?
"OverwriteAuditFile" = Append
"ValidateAutoConfigureLoading" = Warn
   
"SweptSine_Analysis" - 1 entries
"CAEConfiguration" = 
OBJECT ** Job ** (DTJob : Job)
{
  AuditFilename=<Not set>
  Description=
  IgnoreUnusedArguments=False
  MemoryLogging=False
  NumAnalysisThreads=<Not set>
  OverwriteAuditFile=Append
  ValidateAutoConfigureLoading=Warn
  CHILDREN of Job
  {
    OBJECT ** Run1 ** (DTRun : Run)
    {
      Gate=20
      GateUnits=Percent
      NumAnalysisThreads=<Not set>
      TimeHistoryCompression=None
      ATTACHMENTS to Run1
      {
        OBJECT ** AnaDef ** (DTAnalysisDefinition : Analysis definition)
        {
          AnalysisGroups=*
          AutoEliminationMode=False
          CompressionOverride=SameAsRun
          EntitySubsetCombination=<Not set>
          Gate=0
          GateUnits=Percent
          ATTACHMENTS to AnaDef
          {
            OBJECT ** SNEngine ** (DTAnalysisEngineSN : Standard SN analysis engine)
            {
              AngleInterval=10
              BackCalcAccuracy=1
              BackCalcMaxScale=5
              BackCalcMinScale=0.2
              BackCalcMode=None
              BiaxialityGate=20
              BiaxialityThresholdLower=-0.6
              BiaxialityThresholdUpper=0.6
              CertaintyOfSurvival=50
              CheckStaticFailure=False
              CombinationMethod=AbsMaxPrincipal
              CompressByMaxStress=False
              CustomSNMethod=CustomSNTest
              DamageFloor=1E-15
              EventProcessing=Independent
              FatigueReserveFactor=1
              InterpolationLimit=UseMaxCurve
              MaxDamage=1E30
              MeanStressCorrection=Interpolate
              MeanStressCorrectionStrengthParameter=YieldStrength
              MeanStressExponent=1
              MultiAxialAssessment=None
              NonPropFactorThreshold=0.25
              OutputDistributedSource=False
              OutputEventResults=False
              OutputMaterialNames=False
              OutputMaxMin=False
              OutputStats=False
              OutputStressGradientFactors=False
              OutputVibrationStats=False
              SNMethod=MultiRRatioCurve
              ScaleFactor=1
              ScaleNormalStress=False
              SmallCycleCorrection=None
              StaticFailureDamage=2
              StressGradientMethod=VonMises
              StressGradients=Auto
              StressGradientsUser=<Not set>
              TargetDamage=1E-6
              TemperatureInterpolationLimit=UseMaxCurve
              TemperatureSelection=CycleMax
              ZeroCompressiveDamage=Off
              ZeroDamageStressPercent=10
            }
            OBJECT ** MaterialMap ** (DTMaterialMap : Material map)
            {
              CSVFilename=
              DataSetType=nCodeSNRRatioCurveContainer
              DatabaseName=matml
              HideInternalMaterials=True
              MaterialSource=Database
              Permissions=Editable
              SaveMapping=True
              ValidateBeforeRun=False
              WeldLookupFilename=
              CHILDREN of MaterialMap
              {
                OBJECT ** Use materials from Workbench ** (DTMaterialMapLoaderPipe : Material map loader from pipe)
                {
                  Active=True
                  AdditionalDataKeys=Part,Material
                  ClearMap=True
                  MapEntryProperties=
                  MaterialGroupNameKeys=MaterialGroup
                  MaterialNameKey=Material
                }
                OBJECT ** MAT_1 ** (DTMaterialMapEntry : Material map entry)
                {
                  AdhesiveThickness=0.1
                  BondDistanceUnits=mm
                  BondLineOffset=0
                  CutEdgeLocation=None
                  DangVanParameterFilename=<Not set>
                  DatabaseName=<Not set>
                  DefaultMaterial=False
                  DefaultTemperature=0
                  InitialCrackSize=0.4
                  KRoughness=1
                  KTreatment=1
                  KUser=1
                  Material=Test_mat
                  ScaleFactor=1
                  ShapeFactor=<Not set>
                  StressOffset=0
                  StressOffsetUnits=MPa
                  SurfaceRoughness=0
                  SurfaceRoughnessType=Polished
                  WeldDiameter=<Not set>
                  WeldDiameterMethod=Auto
                  WeldDiameterUnits=mm
                  WeldLookupFilename=<Not set>
                }
                OBJECT ** MAT_2 ** (DTMaterialMapEntry : Material map entry)
                {
                  AdhesiveThickness=0.1
                  BondDistanceUnits=mm
                  BondLineOffset=0
                  CutEdgeLocation=None
                  DangVanParameterFilename=<Not set>
                  DatabaseName=<Not set>
                  DefaultMaterial=False
                  DefaultTemperature=0
                  InitialCrackSize=0.4
                  KRoughness=1
                  KTreatment=1
                  KUser=1
                  Material=Test_mat
                  ScaleFactor=1
                  ShapeFactor=<Not set>
                  StressOffset=0
                  StressOffsetUnits=MPa
                  SurfaceRoughness=0
                  SurfaceRoughnessType=Polished
                  WeldDiameter=<Not set>
                  WeldDiameterMethod=Auto
                  WeldDiameterUnits=mm
                  WeldLookupFilename=<Not set>
                }
              }
            }
            OBJECT ** PostProcessorElimination1 ** (DTPostProcessorElimination : Elimination post processor)
            {
              CategoryKeyword=<Not set>
              ColumnsToOutput=
              CountToKeep=1
              EntitySubsetName=gage
              HotSpotPeakDirection=Max
              IncludeAdjacentLocations=False
              KeepMode=Auto
              Limit=<Not set>
              LowerLimit=<Not set>
              MaxNumCategories=100
              MaxNumHotSpots=5
              Mode=HighestCount
              PercentToKeep=10
              ResultKeyword=Damage
              SecondaryFilter=None
              SecondaryLimit=<Not set>
              UpperLimit=<Not set>
            }
          }
        }
      }
    }
    OBJECT ** matml ** (DTMaterialDatabasenCode : nCode material database)
    {
      DatabaseName=C:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\ENGD\material.engd
      DatabaseType=MML
    }
    OBJECT ** Run2 ** (DTRun : Run)
    {
      Gate=0
      GateUnits=Percent
      NumAnalysisThreads=<Not set>
      TimeHistoryCompression=None
      ATTACHMENTS to Run2
      {
        OBJECT ** AnalysisDefinition1 ** (DTAnalysisDefinition : Analysis definition)
        {
          AnalysisGroups=*
          AutoEliminationMode=False
          CompressionOverride=SameAsRun
          EntitySubsetCombination=<Not set>
          Gate=0
          GateUnits=Percent
          ATTACHMENTS to AnalysisDefinition1
          {
            OBJECT ** AnalysisEngineSN1 ** (DTAnalysisEngineSN : Standard SN analysis engine)
            {
              AngleInterval=10
              BackCalcAccuracy=1
              BackCalcMaxScale=5
              BackCalcMinScale=0.2
              BackCalcMode=None
              BiaxialityGate=20
              BiaxialityThresholdLower=-0.6
              BiaxialityThresholdUpper=0.6
              CertaintyOfSurvival=50
              CheckStaticFailure=False
              CombinationMethod=AbsMaxPrincipal
              CompressByMaxStress=False
              CustomSNMethod=None
              DamageFloor=0
              EventProcessing=Independent
              FatigueReserveFactor=1
              InterpolationLimit=UseMaxCurve
              MaxDamage=0
              MeanStressCorrection=Interpolate
              MeanStressCorrectionStrengthParameter=YieldStrength
              MeanStressExponent=1
              MultiAxialAssessment=None
              NonPropFactorThreshold=0.25
              OutputDistributedSource=False
              OutputEventResults=False
              OutputMaterialNames=False
              OutputMaxMin=False
              OutputStats=False
              OutputStressGradientFactors=False
              OutputVibrationStats=False
              SNMethod=MultiRRatioCurve
              ScaleFactor=1
              ScaleNormalStress=False
              SmallCycleCorrection=None
              StaticFailureDamage=2
              StressGradientMethod=VonMises
              StressGradients=Auto
              StressGradientsUser=<Not set>
              TargetDamage=1E-6
              TemperatureInterpolationLimit=UseMaxCurve
              TemperatureSelection=CycleMax
              ZeroCompressiveDamage=Off
              ZeroDamageStressPercent=0
              ATTACHMENTS to AnalysisEngineSN1
              {
                OBJECT ** VibrationPSDOutput1 ** (DTVibrationPSDOutput : Vibration PSD output)
                {
                  ATTACHMENTS to VibrationPSDOutput1
                  {
                    OBJECT ** PSD of Stress ** (DTMultiColumnOutputPipe : Multi-column output to pipe)
                    {
                    }
                  }
                }
                OBJECT ** Cycles Histogram ** (DTHistogramOutputPipe : Histogram output to pipe)
                {
                  HistogramType=Rainflow
                }
                OBJECT ** Damage Histogram ** (DTHistogramOutputPipe : Histogram output to pipe)
                {
                  HistogramType=Damage
                }
              }
            }
            OBJECT ** MaterialMap ** (DTMaterialMap : Material map)
            {
              CSVFilename=
              DataSetType=nCodeSNRRatioCurveContainer
              DatabaseName=matml
              HideInternalMaterials=True
              MaterialSource=Database
              Permissions=Editable
              SaveMapping=True
              ValidateBeforeRun=False
              WeldLookupFilename=
              CHILDREN of MaterialMap
              {
                OBJECT ** Use materials from Workbench ** (DTMaterialMapLoaderPipe : Material map loader from pipe)
                {
                  Active=True
                  AdditionalDataKeys=Part,Material
                  ClearMap=True
                  MapEntryProperties=
                  MaterialGroupNameKeys=MaterialGroup
                  MaterialNameKey=Material
                }
                OBJECT ** MAT_1 ** (DTMaterialMapEntry : Material map entry)
                {
                  AdhesiveThickness=0.1
                  BondDistanceUnits=mm
                  BondLineOffset=0
                  CutEdgeLocation=None
                  DangVanParameterFilename=<Not set>
                  DatabaseName=<Not set>
                  DefaultMaterial=False
                  DefaultTemperature=0
                  InitialCrackSize=0.4
                  KRoughness=1
                  KTreatment=1
                  KUser=1
                  Material=Test_mat
                  ScaleFactor=1
                  ShapeFactor=<Not set>
                  StressOffset=0
                  StressOffsetUnits=MPa
                  SurfaceRoughness=0
                  SurfaceRoughnessType=Polished
                  WeldDiameter=<Not set>
                  WeldDiameterMethod=Auto
                  WeldDiameterUnits=mm
                  WeldLookupFilename=<Not set>
                }
                OBJECT ** MAT_2 ** (DTMaterialMapEntry : Material map entry)
                {
                  AdhesiveThickness=0.1
                  BondDistanceUnits=mm
                  BondLineOffset=0
                  CutEdgeLocation=None
                  DangVanParameterFilename=<Not set>
                  DatabaseName=<Not set>
                  DefaultMaterial=False
                  DefaultTemperature=0
                  InitialCrackSize=0.4
                  KRoughness=1
                  KTreatment=1
                  KUser=1
                  Material=Test_mat
                  ScaleFactor=1
                  ShapeFactor=<Not set>
                  StressOffset=0
                  StressOffsetUnits=MPa
                  SurfaceRoughness=0
                  SurfaceRoughnessType=Polished
                  WeldDiameter=<Not set>
                  WeldDiameterMethod=Auto
                  WeldDiameterUnits=mm
                  WeldLookupFilename=<Not set>
                }
              }
            }
            OBJECT ** gage ** (DTEntitySubsetDynamic : Dynamic entity subset)
            {
              EntityType=Nodes
              ProcessInOrder=False
            }
          }
        }
      }
    }
  }
  ATTACHMENTS to Job
  {
    OBJECT ** VibrationLoad ** (DTLoadProviderVibration : Vibration load provider)
    {
      ActionOnLargePowerRatio=Warn
      ClippingFactor=3
      ComplexAlgorithm=Exact
      ComplexAlgorithmMaxIterations=100
      ComplexAlgorithmPrecision=1E-12
      CycleCountBins=128
      DividerAllStaticLoadCases=<Not set>
      ExposureDuration=1
      Filename=
      FrequencyExtrapolationMethod=UseLimits
      FrequencyInterval=<Not set>
      FrequencySelectionMethod=FRFFrequencies
      InterpolationMethod=LogLog
      LoadingConfigSource=Custom
      LoadingMethod=SineSweep
      MaxFrequency=<Not set>
      MinFrequency=<Not set>
      ModalLoading=False
      NoiseFloor=-120
      NumberOfSweeps=1
      PSDCycleCountMethod=Lalanne
      ResultsSetName=
      ScaleFactorAllStaticLoadCases=<Not set>
      SigmaClipping=None
      SineDwellDurationDays=0
      SineDwellDurationHours=0
      SineDwellDurationSeconds=600
      SineDwellDurationYears=0
      SineDwellFrequency=10
      SineOnRandomAmplitudes=<Not set>
      SineOnRandomCycleCountMethod=NarrowBand
      SineOnRandomFrequencies=<Not set>
      SweepRate=1
      SweepType=LinearHzPerSec
      ATTACHMENTS to VibrationLoad
      {
        OBJECT ** HistogramPipe1 ** (DTHistogramPipe : Histogram input from pipe)
        {
        }
      }
    }
    VibrationLoadCase 1 FELoadCase=1 FELoadCase2=1 Selected Load: Vibration Generator Channel - HistogramPipe1 (c1)
    StaticLoadCase 1 FELoadCase=1 ScaleFactor=1 Divider=1 
    OBJECT ** FEResultsImport ** (DTFEResultsImport : Imported FE results)
    {
      IntermediateFilename=
      NumTranslationProcesses=2
      OneLoadCasePerProcess=False
      SaveIntermediate=True
      TranslateInSeparateProcess=True
      TranslationSplitMethod=Auto
      CHILDREN of FEResultsImport
      {
        OBJECT ** FRF Input ** (DTFEImportResultsSet : FE import results set)
        {
          Description=
          FEFilenames=c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\MECH\file.rst,c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-1\MECH\file.rst
          FEResults=Standard
          IgnoreMidsideNodes=False
          IncludeDisplacements=None
          IncludeEquivalentPlasticStrain=False
          IncludeTemperatures=False
          SelectionGroupType=FEInput
          StateVariableMappingFile=
          UserLoadSetFilename=
          UserLoadSetIDs=
          UserLoadSetType=FromIDs
          VibrationOffset=False
        }
        OBJECT ** Offset Loadcase Input ** (DTFEImportResultsSet : FE import results set)
        {
          Description=<Not set>
          FEFilenames=c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\MECH\file.rst,c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-1\MECH\file.rst
          FEResults=Standard
          IgnoreMidsideNodes=False
          IncludeDisplacements=None
          IncludeEquivalentPlasticStrain=False
          IncludeTemperatures=False
          SelectionGroupType=FEInput
          StateVariableMappingFile=
          UserLoadSetFilename=
          UserLoadSetIDs=
          UserLoadSetType=FromIDs
          VibrationOffset=True
        }
        OBJECT ** AnalysisGroup ** (DTFEImportAnalysisGroup : FE import analysis group)
        {
          AccelerationUnits=mm/s^2
          AdhesiveElementType=Beam
          AllowableFeatureAngle=20
          AverageResultsAtNodes=False
          CriticalDistance=0
          CriticalDistanceMethod=Point
          CriticalDistanceType=AveragedNodeOnElement
          Description=<Not set>
          DistanceUnits=mm
          EntityDataType=Vibration
          ExcludeRigidAttached=False
          ExtrapolationPoints=Two
          ForceUnits=N
          GroupNames=*
          IdentifyFreeEdges=False
          IgnoreZeroData=True
          IncludeSpotWeldCoordinates=False
          IncludeSpotWeldNuggets=True
          LargeDisplacements=False
          LowerFilletOverlapThreshold=30
          MaterialAssignmentGroup=Material
          MaterialOrientationTensor=None
          MaxWeldDepth=0
          MeshQuality=Fine
          MinimumRadiusOfCurvature=0.5
          MomentUnits=N.mm
          NumNotchWeldLines=1
          NumWeldLayers=5
          NumberOfPoints=5
          OffsetMethod=Default
          OffsetType=Ratio
          OffsetValues=0,0,0
          OrientationTensorFile=
          ResolveToLocal=True
          SeamWeldType=Fillet
          SelectionGroupType=FEInput
          SetEntityType=Element
          ShellLayer=TopAndBottom
          SolidLayer=All
          SolidWeldAuto=False
          SolutionLocation=AveragedNodeOnElement
          StateVariableKey=Macro
          StrainGaugeFilename=
          StrainGaugeSource=MetaData
          StrainUnits=strain
          StressGradients=False
          StressUnits=MPa
          SurfaceNodesOnly=True
          SymmetryAxis=Y
          SymmetryDefinitionFilename=
          SymmetryType=None
          TemperatureUnits=deg C
          UnitsDefinition=MPA,MM,N,TNMM,DEGC
          UpperFilletOverlapThreshold=60
          UseShear=False
          UserGroupsToExclude=
          UserSetFilename=
          UserSetIDs=
          UserSetType=FromIDs
          VelocityUnits=mm/s
          VirtualSensorFilename=
          VirtualSensorNodalSum=False
          VirtualSensorSource=MetaData
          WeldDefinitionFilename=
          WeldEndElements=Include
          WeldHotSpotElementType=Solid
          WeldOutputFilename=
          WeldResultLocation=NodeOnElement
        }
      }
    }
    OBJECT ** ResultsHandler ** (DTResultsHandlerFER : FER results handler)
    {
      ColumnsToIgnore=
      ColumnsToSave=ALL
      Filename=
      Overwrite=False
      SaveFile=False
      ATTACHMENTS to ResultsHandler
      {
        OBJECT ** Compressed results (for display) ** (DTPostProcessorPipe : Pipe post processor)
        {
          CategoryKeepCount=1
          CategoryKeyword=
          ChannelPerEvent=False
          Compress=True
          EnableProgressiveUpdate=False
          EquivUnits=Repeats
          IncludeSolids=True
          LayerFullCompression=True
          MinersSum=1
          NumEquivUnits=1
          OutputResultSource=False
          RunColumnOutput=Common
          RunCombination=Worst
          SavePropsToMetadata=False
          ShellLayer=All
          SortKeywords=-Damage
        }
      }
    }
  }
}
   
   
   
Post run audit data
   
Glyph 1 - "VibrationGenerator1"
   
Output channels - 1
Plugs - 1
Plug 1 - "Plug1"
Plug 1 pads - 1
Plug 1 pad 1 channels - 1
Plug 1, Pad 1, Channel 1 = Vibration Generator Channel (channel #1)
   
Properties - 19 entries (post-run state)
AdditionalNumberOfSweeps = 0
EndFrequency = 101
FrequencyStep = 1
InterpolationMethod = Log
Name = sine_sweep
NoiseFloor = -120
NumberOfBins = 1024
PSDUnits = Acceleration
SineAmplitudes = Undefined
SineFrequencies = Undefined
StartFrequency = 1
SweepRate = 1
SweepType = HZ/Sec (Linear)
TestDuration = 100
TestName = Undefined
TestType = Acceleration (g)
Type = SineSweep2
VibrationTable = PropertiesTab
XMLTables = <VibrationTables Version="1.0"><Tables><SineSweep/><SineDwell/><RandomPSD><RandomPSDItem Amplitude="1" Frequency="1"/><RandomPSDItem Amplitude="1" Frequency="1000"/></RandomPSD><SineOnRandom/><SineSweep2><SineSweep2Item Amplitude="0.1" Frequency="1"/><SineSweep2Item Amplitude="1" Frequency="10"/><SineSweep2Item Amplitude="1" Frequency="100"/></SineSweep2></Tables></VibrationTables>

   
Execution time - 0.0015506secs
   
   
Glyph 2 - "Bill_of_Materials_Input"
   
Output channels - 1
Plugs - 1
Plug 1 - "Plug1"
Plug 1 pads - 1
Plug 1 pad 1 channels - 1
Plug 1, Pad 1, Channel 1 =  (channel #1)
   
Properties - 7 entries (post-run state)
CombineAllTests = False
DiscardProcessedTests = False
LoopAllTests = True
MatchingMethod = ChannelNumber
SVDecimalSeparator = 
SVSeparator = 
SaveTestList = False
   
Execution time - 0.004546secs
   
   
Glyph 3 - "Simulation_Input"
Plugs - 1
Plug 1 - "Plug1"
Plug 1 pads - 1
Plug 1 pad 1 channels - 0
   
Properties - 9 entries (post-run state)
CombineTests = True
DiscardProcessedTests = False
ImportUserGroups = False
LoadCaseNumbering = EachFile
LoadCases = Undefined
LoopAllTests = True
SaveTestList = False
StoreDisplayedGroups = False
UserGroupsFilename = Undefined
   
Execution time - 0.0001026secs
   
   
Glyph 4 - "SweptSine_Analysis"
   
Input channels - 2
Sockets - 3
Socket 1 - "FEMetaData"
Socket 1 pads - 2
Socket 2 - "MaterialMapLoader"
Socket 2 pads - 1
Socket 2 pad 1 channels - 1
Socket 2, Pad 1, Channel 1 =  (channel #1)
Socket 3 - "Histogram"
Socket 3 pads - 1
Socket 3 pad 1 channels - 1
Socket 3, Pad 1, Channel 1 = Vibration Generator Channel (channel #1)
   
Output channels - 4
Plugs - 3
Plug 1 - "Results"
Plug 1 pads - 1
Plug 1 pad 1 channels - 1
Plug 1, Pad 1, Channel 1 = Results (channel #1)
Plug 2 - "MultiColumn"
Plug 2 pads - 1
Plug 2 pad 1 channels - 1
Plug 2, Pad 1, Channel 1 = No:6857  Amplitude spectrum of stress (channel #1)
Plug 3 - "Histogram"
Plug 3 pads - 2
Plug 3 pad 1 channels - 1
Plug 3, Pad 1, Channel 1 = No:6857  Sine Sweep (channel #1)
Plug 3 pad 2 channels - 1
Plug 3, Pad 2, Channel 1 = No:6857  Sine Sweep (channel #1)
   
Properties - 23 entries (post-run state)
AnalysisGroup_GroupNames = *
AnalysisGroup_MaterialAssignmentGroup = Material
AnalysisGroup_SelectionGroupType = FEInput
AnalysisGroup_ShellLayer = TopAndBottom
AnalysisGroup_SolutionLocation = AveragedNodeOnElement
AnalysisGroup_UnitsDefinition = MPA,MM,N,TNMM,DEGC
Job_NumAnalysisThreads = ?
LogMessageLimit = 100
LoggingLevel = Info
ResultsUpdateInterval = 10
SNEngine_CertaintyOfSurvival = 50
SNEngine_CombinationMethod = AbsMaxPrincipal
SNEngine_MeanStressCorrection = Interpolate
SNEngine_SNMethod = MultiRRatioCurve
Use materials from Workbench_Active = True
VibrationLoad_FrequencySelectionMethod = FRFFrequencies
VibrationLoad_InterpolationMethod = LogLog
VibrationLoad_LoadingMethod = SineSweep
VibrationLoad_SineDwellDurationSeconds = 600
VibrationLoad_SineDwellFrequency = 10
VibrationLoad_SweepRate = 1
VibrationLoad_SweepType = LinearHzPerSec
matml_DatabaseName = C:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS\ENGD\material.engd
   
Resolved Properties - 1 entries
   
Execution time - 12.3161secs
   
   
Glyph 5 - "HotSpotDetection1"
   
Input channels - 1
Sockets - 2
Socket 1 - "FE Model"
Socket 1 pads - 1
Socket 2 - "CAE Fatigue Results"
Socket 2 pads - 1
Socket 2 pad 1 channels - 1
Socket 2, Pad 1, Channel 1 = Results (channel #1)
   
Output channels - 1
Plugs - 1
Plug 1 - "Hot Spot List"
Plug 1 pads - 1
Plug 1 pad 1 channels - 1
Plug 1, Pad 1, Channel 1 = Hot Spot List (channel #1)
   
Properties - 9 entries (post-run state)
CategoryColumnKeyword = Undefined
ColumnsToOutput = Undefined
EntityType = Auto
HotSpotDataKeyword = Damage
HotSpotPeakDirection = Max
IncludeAdjacentLocations = False
MaxNumCategories = 100
MaxNumHotSpots = 10
ProcessByCategory = False
   
Execution time - 0.0834615secs
   
   
Glyph 6 - "FER_File_Output"
   
Input channels - 1
Sockets - 1
Socket 1 - "S1"
Socket 1 pads - 1
Socket 1 pad 1 channels - 1
Socket 1, Pad 1, Channel 1 = Results (channel #1)
   
Properties - 21 entries (post-run state)
CategoryKeepCount = 1
CategoryKeyword = Undefined
CompressResults = True
EquivUnits = Repeats
EventNaming = Name
ExportCSVDecimalSeparator = 
ExportCSVSeparator = 
GroupType = Property
IncludeSolids = True
MaxGroups = 1000
MinersSum = 1
MultipleEventsSingleODB = False
NodeOnElementCompression = Element
NumEquivUnits = 1
ODBInputFilename = Undefined
OutputFilename = #Test.InputTestInfo.TestName#
OutputFormat = nCode_FER
Overwrite = Yes
Record4ConfigFile = 
ShellLayer = Worst
SortKeywords = -damage
   
Resolved Properties - 1 entries
   
Execution time - 0.456711secs
   
   
Glyph 7 - "HotSpot_List_Output"
   
Input channels - 1
Sockets - 1
Socket 1 - "Socket1"
Socket 1 pads - 1
Socket 1 pad 1 channels - 1
Socket 1, Pad 1, Channel 1 = Hot Spot List (channel #1)
   
Output files - 1
Output file 1 - c:\Users\EdwinRodriguez\Documents\Content\nCodeStat_Harm_init_files\dp0\SYS-2\DL\HotSpot_List.s3m;amc;c1
   
Properties - 13 entries (post-run state)
ASAMDataModel = Undefined
AddToFileList = False
ClearInputGlyphFiles = True
EnumOutput = String
ExportSVDecimalSeparator = 
ExportSVSeparator = 
FileFormat = S3MultiColumn
LoadOutputFilesIntoInputGlyph = 
MetaDataOutput = SaveWithTest
NameText = HotSpot_List
NamingMethod = NewName
Overwrite = Yes
WriteMetadataToSV = False
   
Resolved Properties - 1 entries
   
Execution time - 0.0114602secs
   
   
Glyph 8 - "Fatigue_Results_Display"
   
Input channels - 2
Sockets - 2
Socket 1 - "FE Results"
Socket 1 pads - 1
Socket 1 pad 1 channels - 1
Socket 1, Pad 1, Channel 1 = Results (channel #1)
Socket 2 - "Feature List"
Socket 2 pads - 1
Socket 2 pad 1 channels - 1
Socket 2, Pad 1, Channel 1 = Hot Spot List (channel #1)
   
Properties - 1 entries (post-run state)
ModelFilename = 
   
Resolved Properties - 1 entries
   
Execution time - 1.1289secs
   
   
Glyph 9 - "Swept Sine Display"
   
Input channels - 1
Sockets - 3
Socket 1 - "TSSocket"
Socket 1 pads - 2
Socket 2 - "HistSocket"
Socket 2 pads - 2
Socket 2 pad 1 channels - 1
Socket 2, Pad 1, Channel 1 = Vibration Generator Channel (channel #1)
Socket 3 - "MCSocket"
Socket 3 pads - 2
   
Properties - 30 entries (post-run state)
CursorOutput = None
CursorReceive = None
CursorSend = None
HarmonicXCursors = None
LegendHeightPercent = 25
NameTextInput1 = _in1
NameTextInput2 = _in2
NameTextInput3 = _in3
NameTextInput4 = _in4
NameTextInput5 = _in5
NameTextInput6 = _in6
NameTextInput7 = _in7
NameTextInput8 = _in8
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
NamingMethodInput3 = Suffix
NamingMethodInput4 = Suffix
NamingMethodInput5 = Suffix
NamingMethodInput6 = Suffix
NamingMethodInput7 = Suffix
NamingMethodInput8 = Suffix
NumHistogramInputPads = 2
NumMultiColumnInputPads = 2
NumTsInputPads = 2
NumberPeakCursors = 3
PeakXcursors = None
ShowLegend = False
StoreCursors = False
XCursors = 
YCursors = 
   
Resolved Properties - 1 entries
   
Execution time - 0.0032153secs
   
   
Glyph 10 - "Cycles_Histogram"
   
Input channels - 1
Sockets - 1
Socket 1 - "S1"
Socket 1 pads - 2
Socket 1 pad 1 channels - 1
Socket 1, Pad 1, Channel 1 = No:6857  Sine Sweep (channel #1)
   
Properties - 4 entries (post-run state)
NameTextInput1 = _in1
NameTextInput2 = _in2
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
   
Execution time - 0.0004109secs
   
   
Glyph 11 - "Stress_Amplitude_Spectrum"
   
Input channels - 1
Sockets - 3
Socket 1 - "TSSocket"
Socket 1 pads - 2
Socket 2 - "HistSocket"
Socket 2 pads - 2
Socket 3 - "MCSocket"
Socket 3 pads - 2
Socket 3 pad 1 channels - 1
Socket 3, Pad 1, Channel 1 = No:6857  Amplitude spectrum of stress (channel #1)
   
Properties - 30 entries (post-run state)
CursorOutput = None
CursorReceive = CursorA
CursorSend = CursorA
HarmonicXCursors = None
LegendHeightPercent = 25
NameTextInput1 = _in1
NameTextInput2 = _in2
NameTextInput3 = _in3
NameTextInput4 = _in4
NameTextInput5 = _in5
NameTextInput6 = _in6
NameTextInput7 = _in7
NameTextInput8 = _in8
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
NamingMethodInput3 = Suffix
NamingMethodInput4 = Suffix
NamingMethodInput5 = Suffix
NamingMethodInput6 = Suffix
NamingMethodInput7 = Suffix
NamingMethodInput8 = Suffix
NumHistogramInputPads = 2
NumMultiColumnInputPads = 2
NumTsInputPads = 2
NumberPeakCursors = 3
PeakXcursors = None
ShowLegend = False
StoreCursors = True
XCursors = Undefined
YCursors = Undefined
   
Resolved Properties - 1 entries
   
Execution time - 0.0039293secs
   
   
Glyph 12 - "Damage_Histogram"
   
Input channels - 1
Sockets - 1
Socket 1 - "S1"
Socket 1 pads - 2
Socket 1 pad 1 channels - 1
Socket 1, Pad 1, Channel 1 = No:6857  Sine Sweep (channel #1)
   
Properties - 4 entries (post-run state)
NameTextInput1 = _in1
NameTextInput2 = _in2
NamingMethodInput1 = Suffix
NamingMethodInput2 = Suffix
   
Execution time - 0.0003887secs
   
   
Glyph 13 - "MultiColumnFilter1"
   
Input channels - 1
Sockets - 1
Socket 1 - "Socket1"
Socket 1 pads - 1
Socket 1 pad 1 channels - 1
Socket 1, Pad 1, Channel 1 = Results (channel #1)
   
Output channels - 1
Plugs - 1
Plug 1 - "Plug1"
Plug 1 pads - 1
Plug 1 pad 1 channels - 1
Plug 1, Pad 1, Channel 1 = Results (channel #1)
   
Properties - 7 entries (post-run state)
Channels = Undefined
ColumnsToExclude = Undefined
ColumnsToInclude = NodeID,Damage,Life
FilterCaseSensitive = False
FilterColumn = Undefined
FilterComparison = =
FilterValue = Undefined
   
Resolved Properties - 1 entries
   
Execution time - 0.003151secs
   
   
Glyph 14 - "CSV_File_Output"
   
Input channels - 1
Sockets - 1
Socket 1 - "S1"
Socket 1 pads - 1
Socket 1 pad 1 channels - 1
Socket 1, Pad 1, Channel 1 = Results (channel #1)
   
Properties - 21 entries (post-run state)
CategoryKeepCount = 1
CategoryKeyword = Undefined
CompressResults = True
EquivUnits = Repeats
EventNaming = Name
ExportCSVDecimalSeparator = 
ExportCSVSeparator = 
GroupType = Property
IncludeSolids = True
MaxGroups = 1000
MinersSum = 1
MultipleEventsSingleODB = False
NodeOnElementCompression = Element
NumEquivUnits = 1
ODBInputFilename = Undefined
OutputFilename = dl_results
OutputFormat = CSV
Overwrite = Yes
Record4ConfigFile = 
ShellLayer = Worst
SortKeywords = -damage
   
Resolved Properties - 1 entries
   
Execution time - 0.186852secs
   
   
Glyph 15 - "DX_parameters"
Plugs - 1
Plug 1 - "Output"
Plug 1 pads - 1
Plug 1 pad 1 channels - 0
   
Properties - 4 entries (post-run state)
HideSetupTabs = True
Parameter_per_group = False
Parameter_type = life
Properties = <Properties><Property help="If True, a parameter for each material group is exported. If False a single parameter for the entire model is exported." name="Parameter_per_group" type="boolean" mandatory="true" description="Export a parameter for each material group, or a single parameter for the model"/><Property help="The worst result of this type will be passed back to DesignExplorer. Fatigue analyses for damage can export either life or damage. Backcalculation analyses can export scalefactor, and DangVan can export safetyfactor. On a dutycycle run, the total schedule results is used." name="Parameter_type" type="enum" enumopts="damage,life,safetyfactor,scalefactor" mandatory="true" description="Type of fatigue result to pass to DesignExplorer"/></Properties>
   
Execution time - 0.0104844secs
   
   
Glyph 16 - "Design Explorer Output1"
   
Input channels - 1
Sockets - 1
Socket 1 - "Linked to SGInput1"
Socket 1 pads - 2
Socket 1 pad 1 channels - 1
Socket 1, Pad 1, Channel 1 = Results (channel #1)
   
Properties - 5 entries (post-run state)
BitmapFileName = SuperGlyph
IconFileName = SuperGlyph
Locked = False
Verbose = True
   
Execution time - 0.422938secs
   
   
Glyph 17 - "DataValuesDisplay"
   
Input channels - 1
Sockets - 1
Socket 1 - "S1"
Socket 1 pads - 4
Socket 1 pad 3 channels - 1
Socket 1, Pad 3, Channel 1 = Results (channel #1)
Plugs - 1
Plug 1 - "Plug1"
   
Properties - 33 entries (post-run state)
2DHistogramVerticalFormat = True
ChannelsToDisplay = Undefined
ColumnLabel = AxisTitle
Columns = 
ColumnsToColour = 
DisplayMode = Mag/Phase
EqualsColour = LightGreen
EqualsTolerance = 1E-4
EqualsValue = ?
ExportCSVDecimalSeparator = 
ExportCSVSeparator = 
ExportNameText = Undefined
ExportNamingMethod = Suffix
ExportType = None
HistogramBinLabels = BinCentre
IntegerFormat = Decimal
IntervalUnits = Point
LowerGate = ?
LowerGateColour = Blue
MaximumValueColour = Undefined
MinimumValueColour = Undefined
MissingValuesSpace = True
NumberSigFig = 4
Overwrite = Ask
PointIncrementValue = 10
ReverseYAxis = False
ShowColumnKeywords = False
ShowColumnTypes = False
TransposeXY = Normal
UTCFormat = Local
UpperGate = ?
UpperGateColour = Red
XAxisUnitsIncrementValue = 1
   
Resolved Properties - 1 entries
   
Execution time - 0.0131613secs
   
   
Single run - PASSED
End time - 15-Aug-2025 15:16:30
   
   
   
Product         GlyphWorks V25.0.0 Release Build 431
Platform        Windows64
abcdlib         V25.0 A01 Jan 14 2025 12:42:50
ailib           V25.0 A01 Jan 14 2025 12:43:34
anslib          V25.0 A01 Jan 14 2025 12:43:19
asamlib         V25.0 A01 Jan 14 2025 13:07:33
atlib           V25.0 A01 Jan 14 2025 12:51:03
CBLib           V25.0 A01 Jan 14 2025 12:43:46
cgdlib          V25.0 A01 Jan 14 2025 12:48:23
cgflib          V25.0 A01 Jan 14 2025 12:41:16
cgolib          V25.0 A01 Jan 14 2025 12:48:07
cgrlib          V25.0 A01 Jan 14 2025 12:47:43
cpputil         V25.0 A01 Jan 14 2025 12:34:31
dglib           V25.0 A01 Jan 14 2025 12:50:00
dmilib          V25.0 A01 Jan 14 2025 12:35:37
dtlib           V25.0 A01 Jan 14 2025 12:47:07
extlib          V25.0 A01 Jan 14 2025 12:32:12
fatlib          V25.0 A01 Jan 14 2025 12:39:41
FDLib           V25.0 A01 Jan 14 2025 12:44:23
fedlib          V25.0 A01 Jan 14 2025 12:53:52
feilib          V25.0 A01 Jan 14 2025 12:43:08
feimportlib (ANSYS) V25.0 A01 Jan 14 2025 12:46:38
ferlib          V25.0 A01 Jan 14 2025 12:37:58
fiolib          V25.0 A01 Jan 14 2025 12:42:00
flowproc        V25.0 A01 Jan 14 2025 13:28:42
FSLib           V25.0 A01 Jan 14 2025 12:37:05
FVLib           V25.0 A01 Jan 14 2025 12:56:58
GlyphEngine01   V25.0 A01 Jan 14 2025 12:59:10
GlyphEngine02   V25.0 A01 Jan 14 2025 12:59:49
GlyphEngine03   V25.0 A01 Jan 14 2025 13:00:38
GlyphEngine04   V25.0 A01 Jan 14 2025 13:01:39
GlyphEngine06   V25.0 A01 Jan 14 2025 13:02:36
GlyphEngine07   V25.0 A01 Jan 14 2025 13:03:02
GlyphEngine08   V25.0 A01 Jan 14 2025 13:03:23
GlyphEngine09   V25.0 A01 Jan 14 2025 13:03:48
GlyphEngine10   V25.0 A01 Jan 14 2025 13:04:14
GlyphEngine13   V25.0 A01 Jan 14 2025 13:04:39
GlyphEngine14   V25.0 A01 Jan 14 2025 13:05:28
GlyphEngine15   V25.0 A01 Jan 14 2025 13:05:56
GlyphEngine16   V25.0 A01 Jan 14 2025 13:06:24
grlib           V25.0 A01 Jan 14 2025 12:51:53
gutlib          V25.0 A01 Jan 14 2025 12:55:50
iceintlib       V25.0 A01 Jan 14 2025 12:50:33
IXDLib          V25.0 A01 Jan 14 2025 12:35:52
jprolib         V25.0 A01 Jan 14 2025 12:42:35
lican           V25.0 A01 Jan 14 2025 12:30:34
licnc           V25.0 A01 Jan 14 2025 12:30:19
licsh           V25.0 A01 Jan 14 2025 12:30:10
maplib          V25.0 A01 Jan 14 2025 12:35:25
matdblib        V25.0 A01 Jan 14 2025 12:38:15
materials       V25.0 A01 Jan 14 2025 12:49:26
mcxlib          V25.0 A01 Jan 14 2025 12:32:51
mthlib          V25.0 A01 Jan 14 2025 12:35:14
mtlib           V25.0 A01 Jan 14 2025 12:33:48
ncmpilib        V25.0 A01 Jan 14 2025 12:32:18
ncxml           V25.0 A01 Jan 14 2025 12:30:42
nmxfiolib       V25.0 A01 Jan 14 2025 12:37:45
nulib           V25.0 A01 Jan 14 2025 12:34:46
NXLib           V25.0 A01 Jan 14 2025 12:33:01
ProgramEngine00 V25.0 A01 Jan 14 2025 13:06:46
pylib           V25.0 A01 Jan 14 2025 12:33:57
QCLib           V25.0 A01 Jan 14 2025 12:55:21
qtutil          V25.0 A01 Jan 14 2025 12:48:50
QXLib           V25.0 A01 Jan 14 2025 12:45:08
S3Lib           V25.0 A01 Jan 14 2025 12:33:22
sielib          V25.0 A01 Jan 14 2025 12:37:35
siglib          V25.0 A01 Jan 14 2025 12:40:54
utlib (ANSYS)   V25.0 A01 Jan 14 2025 12:28:47
xllib           V25.0 A01 Jan 14 2025 12:31:01
